!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v5.0.1.3581
!
!  Generated Wed Oct 19 16:51:17 2011 PDT by vadim
!
! Compiled for pix 7.0
! Outbound ACLs: supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: yes
! Assume firewall is part of any: yes
!
!# files: * cluster1-1_pix2.fw
!
!

! pix2::: warning: Interface Ethernet0 has vlan subinterfaces, it can not be used for ACL. Marking this interface "unprotected" to exclude it.

!
! Prolog script:
!

!
! End of prolog script:
!




hostname pix2

interface Ethernet1
  nameif inside
  ip address 10.3.14.207 255.255.255.0  standby 10.3.14.206 
  security-level 100
exit

interface Ethernet0
  no nameif
  no ip address
  no security-level
exit

interface Ethernet2
  description LAN/STATE Failover Interface
  no nameif
exit

interface Ethernet0.101
  vlan 101
  nameif outside
  ip address 192.0.2.254 255.255.255.0  standby 192.0.2.253 
  security-level 0
exit

interface Ethernet0.102
  vlan 102
  nameif dmz20
  ip address 10.0.0.254 255.255.255.0  standby 10.0.0.253 
  security-level 20
exit


failover lan unit secondary
failover lan interface failover Ethernet2 
failover lan enable
failover key super_secret
failover interface ip failover 172.17.1.253 255.255.255.252 standby 172.17.1.254
failover link failover Ethernet2
failover interface ip failover 172.17.1.253 255.255.255.252 standby 172.17.1.254
failover


no logging buffered
no logging console
no logging timestamp
no logging on


timeout xlate 0:0:30 
timeout conn 0:0:0 
timeout udp 0:0:0 
timeout sunrpc 0:0:0 
timeout h323 0:0:0 
timeout sip 0:0:0 
timeout sip_media 0:0:0 
timeout half-closed 0:0:0 
timeout uauth 0:0:0 


clear config ssh
aaa authentication ssh console LOCAL

clear config snmp-server
no snmp-server enable traps

clear config ntp


no service resetinbound
no service resetoutside
no sysopt connection timewait
no sysopt nodnsalias inbound
no sysopt nodnsalias outbound


class-map inspection_default
  match default-inspection-traffic

policy-map global_policy
  class inspection_default

service-policy global_policy global


!################

clear xlate
clear config static
clear config global
clear config nat
clear config access-list
clear config icmp
clear config telnet
clear config object-group
clear config object

object-group network id56590X61097.src.net.0
  network-object host 10.3.14.206 
  network-object host 10.3.14.207 
exit

object-group network id56590X61097.src.net.1
  network-object host 172.17.1.253 
  network-object host 172.17.1.254 
  network-object host 192.0.2.253 
  network-object host 192.0.2.254 
exit

object-group network id56590X61097.src.net.2
  network-object host 10.0.0.253 
  network-object host 10.0.0.254 
exit

object-group network id56627X61097.src.net.0
  network-object host 172.17.1.253 
  network-object host 192.0.2.253 
exit

! 
! Rule  0 (Ethernet0.101)
! anti spoofing rule
access-list outside_in deny   ip object-group id56590X61097.src.net.0 any log 3 interval 300
access-list outside_in deny   ip object-group id56590X61097.src.net.1 any log 3 interval 300
access-list outside_in deny   ip object-group id56590X61097.src.net.2 any log 3 interval 300
access-list outside_in deny   ip 10.3.14.0 255.255.255.0 any log 3 interval 300
! 
! Rule  1 (global)
! SSH Access to firewall is permitted
! only from internal network
ssh 10.3.14.0 255.255.255.0 inside
! 
! Rule  2 (global)
ssh 10.3.14.0 255.255.255.0 inside
! 
! Rule  3 (global)
! Firewall uses one of the machines
! on internal network for DNS
access-list inside_out permit udp host 10.3.14.206 10.3.14.0 255.255.255.0 eq 53 log 3 interval 300
access-list inside_out permit udp object-group id56627X61097.src.net.0 10.3.14.0 255.255.255.0 eq 53 log 3 interval 300
access-list inside_out permit udp host 10.0.0.253 10.3.14.0 255.255.255.0 eq 53 log 3 interval 300
! 
! Rule  4 (global)
! Firewall uses one of the machines
! on internal network for DNS
access-list inside_out permit udp object-group id56590X61097.src.net.0 10.3.14.0 255.255.255.0 eq 53 log 3 interval 300
access-list inside_out permit udp object-group id56590X61097.src.net.1 10.3.14.0 255.255.255.0 eq 53 log 3 interval 300
access-list inside_out permit udp object-group id56590X61097.src.net.2 10.3.14.0 255.255.255.0 eq 53 log 3 interval 300
! 
! Rule  5 (global)
! All other attempts to connect to
! the firewall are denied and logged
access-list inside_in deny   ip any object-group id56590X61097.src.net.0 log 3 interval 300
access-list inside_in deny   ip any object-group id56590X61097.src.net.1 log 3 interval 300
access-list inside_in deny   ip any object-group id56590X61097.src.net.2 log 3 interval 300
! 
! Rule  6 (global)
access-list inside_in permit ip 10.3.14.0 255.255.255.0 any 
access-list inside_out permit ip 10.3.14.0 255.255.255.0 any 
! 
! Rule  7 (global)
access-list inside_in deny   ip any any log 3 interval 300
access-list inside_out deny   ip any any log 3 interval 300


access-group inside_in in interface inside
access-group inside_out out interface inside
access-group outside_in in interface outside

! 
! Rule  0 (NAT)
global (outside) 1 interface
access-list id56689X61097.0 permit ip 10.3.14.0 255.255.255.0  any 
nat (inside) 1 access-list id56689X61097.0 tcp 0 0



!
! Epilog script:
!

! End of epilog script:
!
