#!/bin/sh 
#
#  This is automatically generated file. DO NOT MODIFY !
#
#  Firewall Builder  fwb_ipt v5.0.2.3596
#
#  Generated Sun Mar 18 21:16:07 2012 PDT by vadim
#
# files: * firewall1.fw /etc/fw/firewall1.fw
#
# Compiled for iptables (any version)
#
# this object is used to test all kinds of negation in policy and NAT rules.
# Assume firewall is part of any is ON




FWBDEBUG=""

PATH="/sbin:/usr/sbin:/bin:/usr/bin:${PATH}"
export PATH



LSMOD="/sbin/lsmod"
MODPROBE="/sbin/modprobe"
IPTABLES="/sbin/iptables"
IP6TABLES="/sbin/ip6tables"
IPTABLES_RESTORE="/sbin/iptables-restore"
IP6TABLES_RESTORE="/sbin/ip6tables-restore"
IP="/sbin/ip"
IFCONFIG="/sbin/ifconfig"
VCONFIG="/sbin/vconfig"
BRCTL="/sbin/brctl"
IFENSLAVE="/sbin/ifenslave"
IPSET="/usr/sbin/ipset"
LOGGER="/usr/bin/logger"

log() {
    echo "$1"
    which "$LOGGER" >/dev/null 2>&1 && $LOGGER -p info "$1"
}

getInterfaceVarName() {
    echo $1 | sed 's/\./_/'
}

getaddr_internal() {
    dev=$1
    name=$2
    af=$3
    L=$($IP $af addr show dev $dev |  sed -n '/inet/{s!.*inet6* !!;s!/.*!!p}' | sed 's/peer.*//')
    test -z "$L" && { 
        eval "$name=''"
        return
    }
    eval "${name}_list=\"$L\"" 
}

getnet_internal() {
    dev=$1
    name=$2
    af=$3
    L=$($IP route list proto kernel | grep $dev | grep -v default |  sed 's! .*$!!')
    test -z "$L" && { 
        eval "$name=''"
        return
    }
    eval "${name}_list=\"$L\"" 
}


getaddr() {
    getaddr_internal $1 $2 "-4"
}

getaddr6() {
    getaddr_internal $1 $2 "-6"
}

getnet() {
    getnet_internal $1 $2 "-4"
}

getnet6() {
    getnet_internal $1 $2 "-6"
}

# function getinterfaces is used to process wildcard interfaces
getinterfaces() {
    NAME=$1
    $IP link show | grep ": $NAME" | while read L; do
        OIFS=$IFS
        IFS=" :"
        set $L
        IFS=$OIFS
        echo $2
    done
}

diff_intf() {
    func=$1
    list1=$2
    list2=$3
    cmd=$4
    for intf in $list1
    do
        echo $list2 | grep -q $intf || {
        # $vlan is absent in list 2
            $func $intf $cmd
        }
    done
}

find_program() {
  PGM=$1
  which $PGM >/dev/null 2>&1 || {
    echo "\"$PGM\" not found"
    exit 1
  }
}
check_tools() {
  find_program which
  find_program $IPTABLES 
  find_program $IP 
}
reset_iptables_v4() {
  $IPTABLES -P OUTPUT  DROP
  $IPTABLES -P INPUT   DROP
  $IPTABLES -P FORWARD DROP

cat /proc/net/ip_tables_names | while read table; do
  $IPTABLES -t $table -L -n | while read c chain rest; do
      if test "X$c" = "XChain" ; then
        $IPTABLES -t $table -F $chain
      fi
  done
  $IPTABLES -t $table -X
done
}

reset_iptables_v6() {
  $IP6TABLES -P OUTPUT  DROP
  $IP6TABLES -P INPUT   DROP
  $IP6TABLES -P FORWARD DROP

cat /proc/net/ip6_tables_names | while read table; do
  $IP6TABLES -t $table -L -n | while read c chain rest; do
      if test "X$c" = "XChain" ; then
        $IP6TABLES -t $table -F $chain
      fi
  done
  $IP6TABLES -t $table -X
done
}


P2P_INTERFACE_WARNING=""

missing_address() {
    address=$1
    cmd=$2

    oldIFS=$IFS
    IFS="@"
    set $address
    addr=$1
    interface=$2
    IFS=$oldIFS



    $IP addr show dev $interface | grep -q POINTOPOINT && {
        test -z "$P2P_INTERFACE_WARNING" && echo "Warning: Can not update address of interface $interface. fwbuilder can not manage addresses of point-to-point interfaces yet"
        P2P_INTERFACE_WARNING="yes"
        return
    }

    test "$cmd" = "add" && {
      echo "# Adding ip address: $interface $addr"
      echo $addr | grep -q ':' && {
          $FWBDEBUG $IP addr $cmd $addr dev $interface
      } || {
          $FWBDEBUG $IP addr $cmd $addr broadcast + dev $interface
      }
    }

    test "$cmd" = "del" && {
      echo "# Removing ip address: $interface $addr"
      $FWBDEBUG $IP addr $cmd $addr dev $interface || exit 1
    }

    $FWBDEBUG $IP link set $interface up
}

list_addresses_by_scope() {
    interface=$1
    scope=$2
    ignore_list=$3
    $IP addr ls dev $interface | \
      awk -v IGNORED="$ignore_list" -v SCOPE="$scope" \
        'BEGIN {
           split(IGNORED,ignored_arr);
           for (a in ignored_arr) {ignored_dict[ignored_arr[a]]=1;}
         }
         (/inet |inet6 / && $0 ~ SCOPE && !($2 in ignored_dict)) {print $2;}' | \
        while read addr; do
          echo "${addr}@$interface"
	done | sort
}


update_addresses_of_interface() {
    ignore_list=$2
    set $1 
    interface=$1 
    shift

    FWB_ADDRS=$(
      for addr in $*; do
        echo "${addr}@$interface"
      done | sort
    )

    CURRENT_ADDRS_ALL_SCOPES=""
    CURRENT_ADDRS_GLOBAL_SCOPE=""

    $IP link show dev $interface >/dev/null 2>&1 && {
      CURRENT_ADDRS_ALL_SCOPES=$(list_addresses_by_scope $interface 'scope .*' "$ignore_list")
      CURRENT_ADDRS_GLOBAL_SCOPE=$(list_addresses_by_scope $interface 'scope global' "$ignore_list")
    } || {
      echo "# Interface $interface does not exist"
      # Stop the script if we are not in test mode
      test -z "$FWBDEBUG" && exit 1
    }

    diff_intf missing_address "$FWB_ADDRS" "$CURRENT_ADDRS_ALL_SCOPES" add
    diff_intf missing_address "$CURRENT_ADDRS_GLOBAL_SCOPE" "$FWB_ADDRS" del
}

clear_addresses_except_known_interfaces() {
    $IP link show | sed 's/://g' | awk -v IGNORED="$*" \
        'BEGIN {
           split(IGNORED,ignored_arr);
           for (a in ignored_arr) {ignored_dict[ignored_arr[a]]=1;}
         }
         (/state/ && !($2 in ignored_dict)) {print $2;}' | \
         while read intf; do
            echo "# Removing addresses not configured in fwbuilder from interface $intf"
            $FWBDEBUG $IP addr flush dev $intf scope global
            $FWBDEBUG $IP link set $intf down
         done
}

check_file() {
    test -r "$2" || {
        echo "Can not find file $2 referenced by address table object $1"
        exit 1
    }
}

check_run_time_address_table_files() {
    :
    
}

load_modules() {
    :
    
}

verify_interfaces() {
    :
    
}

prolog_commands() {
    echo "Running prolog script"
    
}

epilog_commands() {
    echo "Running epilog script"
    
}

run_epilog_and_exit() {
    epilog_commands
    exit $1
}

configure_interfaces() {
    :
    # Configure interfaces
    # See http://bugs.debian.org/cgi-bin/bugreport.cgi?bug=429689
    # this ensures that secondary ip address is "promoted" to primary
    # when primary address is deleted, instead of deleting both
    # primary and secondary addresses. It looks like this is only
    # available starting from Linux 2.6.16 
    test -f /proc/sys/net/ipv4/conf/all/promote_secondaries && \
        echo 1 >  /proc/sys/net/ipv4/conf/all/promote_secondaries
    update_addresses_of_interface "eth0 192.168.1.1/24 192.168.1.0/24" ""
    update_addresses_of_interface "eth1 22.22.22.22/24 22.22.22.23/24" ""
    update_addresses_of_interface "eth2 192.168.2.1/24 192.168.2.0/24" ""
    update_addresses_of_interface "lo 127.0.0.1/8" ""
    update_addresses_of_interface "eth3 22.22.23.23/24" ""
}

script_body() {
    echo 30 > /proc/sys/net/ipv4/tcp_fin_timeout 
     echo 1800 > /proc/sys/net/ipv4/tcp_keepalive_intvl 


    # ================ IPv4


    # ================ Table 'filter', automatic rules
    # accept established sessions
    $IPTABLES -A INPUT   -m state --state ESTABLISHED,RELATED -j ACCEPT 
    $IPTABLES -A OUTPUT  -m state --state ESTABLISHED,RELATED -j ACCEPT 
    $IPTABLES -A FORWARD -m state --state ESTABLISHED,RELATED -j ACCEPT 
    # drop packets that do not match any valid state and log them
    $IPTABLES -N drop_invalid
    $IPTABLES -A OUTPUT   -m state --state INVALID  -j drop_invalid 
    $IPTABLES -A INPUT    -m state --state INVALID  -j drop_invalid 
    $IPTABLES -A FORWARD  -m state --state INVALID  -j drop_invalid 
    $IPTABLES -A drop_invalid -j LOG --log-level debug --log-prefix "INVALID state -- DENY "
    $IPTABLES -A drop_invalid -j DROP


    # ================ Table 'nat',  rule set NAT
    # 
    # Rule 0 (NAT)
    # 
    echo "Rule 0 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING  -s 192.168.1.0/24  -d 192.168.2.0/24  -j ACCEPT
    $IPTABLES -t nat -A PREROUTING  -s 192.168.1.0/24  -d 192.168.2.0/24  -j ACCEPT
    # 
    # Rule 1 (NAT)
    # 
    echo "Rule 1 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth+   -s 192.168.1.10  -j SNAT --to-source 22.22.22.23
    # 
    # Rule 2 (NAT)
    # 
    echo "Rule 2 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth+   -s ! 192.168.1.0/24  -d 200.200.200.200  -j SNAT --to-source 22.22.22.23
    # 
    # Rule 3 (NAT)
    # 
    echo "Rule 3 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth+  -p tcp -m tcp  -s ! 192.168.1.0/24   -d 200.200.200.200  --dport 80 -j SNAT --to-source 22.22.22.23
    # 
    # Rule 4 (NAT)
    # 
    echo "Rule 4 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth1   -s 192.168.1.0/24  -j SNAT --to-source 22.22.22.22
    $IPTABLES -t nat -A POSTROUTING -o eth3   -s 192.168.1.0/24  -j SNAT --to-source 22.22.23.23
    $IPTABLES -t nat -A POSTROUTING -o eth2   -s 192.168.1.0/24  -j SNAT --to-source 192.168.2.1
    # 
    # Rule 5 (NAT)
    # 
    echo "Rule 5 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth1   -s 192.168.1.0/24  -j SNAT --to-source 22.22.22.22
    $IPTABLES -t nat -A POSTROUTING -o eth3   -s 192.168.1.0/24  -j SNAT --to-source 22.22.23.23
    # 
    # Rule 6 (NAT)
    # 
    echo "Rule 6 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth1   -s 192.168.1.0/24  -d ! 192.168.2.0/24  -j SNAT --to-source 22.22.22.22
    $IPTABLES -t nat -A POSTROUTING -o eth3   -s 192.168.1.0/24  -d ! 192.168.2.0/24  -j SNAT --to-source 22.22.23.23
    # 
    # Rule 7 (NAT)
    # 
    echo "Rule 7 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth1  -p tcp -m tcp  -s 192.168.1.0/24   -d ! 192.168.2.0/24  --dport 80 -j SNAT --to-source 22.22.22.22
    $IPTABLES -t nat -A POSTROUTING -o eth3  -p tcp -m tcp  -s 192.168.1.0/24   -d ! 192.168.2.0/24  --dport 80 -j SNAT --to-source 22.22.23.23
    # 
    # Rule 8 (NAT)
    # 
    echo "Rule 8 (NAT)"
    # 
    $IPTABLES -t nat -N Cid3CCA1B57.0
    $IPTABLES -t nat -A POSTROUTING -o eth1   -s 192.168.1.0/24  -j Cid3CCA1B57.0
    $IPTABLES -t nat -A POSTROUTING -o eth3   -s 192.168.1.0/24  -j Cid3CCA1B57.0
    $IPTABLES -t nat -A POSTROUTING -o eth2   -s 192.168.1.0/24  -j Cid3CCA1B57.0
    $IPTABLES -t nat -A Cid3CCA1B57.0  -d 192.168.1.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3CCA1B57.0  -d 192.168.2.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3CCA1B57.0  -j SNAT --to-source 22.22.22.22
    $IPTABLES -t nat -A Cid3CCA1B57.0  -j SNAT --to-source 22.22.23.23
    $IPTABLES -t nat -A Cid3CCA1B57.0  -j SNAT --to-source 192.168.2.1
    # 
    # Rule 9 (NAT)
    # 
    echo "Rule 9 (NAT)"
    # 
    $IPTABLES -t nat -N Cid3EB38983.0
    $IPTABLES -t nat -A POSTROUTING -o eth1   -s 192.168.1.0/24  -j Cid3EB38983.0
    $IPTABLES -t nat -A POSTROUTING -o eth3   -s 192.168.1.0/24  -j Cid3EB38983.0
    $IPTABLES -t nat -A POSTROUTING -o eth2   -s 192.168.1.0/24  -j Cid3EB38983.0
    $IPTABLES -t nat -A Cid3EB38983.0  -d 192.168.1.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3EB38983.0  -d 192.168.2.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3EB38983.0  -j SNAT --to-source 22.22.22.22
    $IPTABLES -t nat -A Cid3EB38983.0  -j SNAT --to-source 22.22.23.23
    $IPTABLES -t nat -A Cid3EB38983.0  -j SNAT --to-source 192.168.2.1
    # 
    # Rule 10 (NAT)
    # 
    echo "Rule 10 (NAT)"
    # 
    $IPTABLES -t nat -A POSTROUTING -o eth1   -s ! 192.168.2.0/24  -j SNAT --to-source 22.22.22.22
    $IPTABLES -t nat -A POSTROUTING -o eth3   -s ! 192.168.2.0/24  -j SNAT --to-source 22.22.23.23
    $IPTABLES -t nat -A POSTROUTING -o eth0   -s ! 192.168.2.0/24  -j SNAT --to-source 192.168.1.1
    # 
    # Rule 11 (NAT)
    # 
    echo "Rule 11 (NAT)"
    # 
    $IPTABLES -t nat -N Cid3BD8D94B.0
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp  -s 192.168.1.0/24   --dport 80 -j Cid3BD8D94B.0
    $IPTABLES -t nat -A Cid3BD8D94B.0  -d 22.22.22.22  -j RETURN
    $IPTABLES -t nat -A Cid3BD8D94B.0  -d 22.22.23.23  -j RETURN
    $IPTABLES -t nat -A Cid3BD8D94B.0  -d 192.168.1.1  -j RETURN
    $IPTABLES -t nat -A Cid3BD8D94B.0  -d 192.168.2.1  -j RETURN
    $IPTABLES -t nat -A Cid3BD8D94B.0 -p tcp -m tcp   --dport 80 -j REDIRECT --to-ports 3128
    # 
    # Rule 12 (NAT)
    # 
    echo "Rule 12 (NAT)"
    # 
    $IPTABLES -t nat -N Cid3BD8D9DD.0
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp  -s 192.168.1.0/24   --dport 80 -j Cid3BD8D9DD.0
    $IPTABLES -t nat -A Cid3BD8D9DD.0  -d 192.168.1.1  -j RETURN
    $IPTABLES -t nat -A Cid3BD8D9DD.0 -p tcp -m tcp   --dport 80 -j REDIRECT --to-ports 3128
    # 
    # Rule 13 (NAT)
    # 
    echo "Rule 13 (NAT)"
    # 
    $IPTABLES -t nat -N Cid3BBC0EA4.0
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp  -s 192.168.1.10   --dport 80 -j Cid3BBC0EA4.0
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp  -s 192.168.1.20   --dport 80 -j Cid3BBC0EA4.0
    $IPTABLES -t nat -A Cid3BBC0EA4.0  -d 192.168.1.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3BBC0EA4.0  -d 192.168.2.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3BBC0EA4.0 -p tcp -m tcp   --dport 80 -j REDIRECT --to-ports 3128
    # 
    # Rule 14 (NAT)
    # 
    echo "Rule 14 (NAT)"
    # 
    $IPTABLES -t nat -N Cid3BBC0F93.0
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp   -d 192.168.1.0/24  --dport 80 -j Cid3BBC0F93.0
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp   -d 192.168.2.0/24  --dport 80 -j Cid3BBC0F93.0
    $IPTABLES -t nat -A Cid3BBC0F93.0  -s 192.168.1.10  -j RETURN
    $IPTABLES -t nat -A Cid3BBC0F93.0  -s 192.168.1.20  -j RETURN
    $IPTABLES -t nat -A Cid3BBC0F93.0 -p tcp -m tcp   --dport 80 -j REDIRECT --to-ports 3128
    # 
    # Rule 15 (NAT)
    # 
    echo "Rule 15 (NAT)"
    # 
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp  -s ! 192.168.1.10   --dport 80 -j REDIRECT --to-ports 3128
    # 
    # Rule 16 (NAT)
    # 
    echo "Rule 16 (NAT)"
    # 
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp   -d 22.22.22.23  --dport 4000:4010 -j DNAT --to-destination 192.168.1.10
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp  --sport 5000  -d 22.22.22.23  --dport 5000:5010 -j DNAT --to-destination 192.168.1.10
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp  --sport 9000  -d 22.22.22.23  -j DNAT --to-destination 192.168.1.10
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp -m multiport   -d 22.22.22.23  --dports 6667,3128 -j DNAT --to-destination 192.168.1.10
    # 
    # Rule 17 (NAT)
    # 
    echo "Rule 17 (NAT)"
    # 
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp   -d 192.168.1.0/24  --dport 80 -j DNAT --to-destination :3128
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp   -d 192.168.2.0/24  --dport 80 -j DNAT --to-destination :3128
    # 
    # Rule 18 (NAT)
    # 
    echo "Rule 18 (NAT)"
    # 
    $IPTABLES -t nat -N Cid3EB38A91.0
    $IPTABLES -t nat -A PREROUTING -p tcp -m tcp   --dport 80 -j Cid3EB38A91.0
    $IPTABLES -t nat -A Cid3EB38A91.0  -d 192.168.1.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3EB38A91.0  -d 192.168.2.0/24  -j RETURN
    $IPTABLES -t nat -A Cid3EB38A91.0 -p tcp -m tcp   --dport 80 -j DNAT --to-destination :3128



    # ================ Table 'filter', rule set GOOD_GUYS
    # 
    # Rule GOOD_GUYS 0 (global)
    # 
    echo "Rule GOOD_GUYS 0 (global)"
    # 
    $IPTABLES -N GOOD_GUYS
    $IPTABLES -N Cid40710X74808.0
    $IPTABLES -A GOOD_GUYS  -j Cid40710X74808.0
    $IPTABLES -A Cid40710X74808.0  -s 1.1.1.0/24   -j RETURN
    $IPTABLES -A Cid40710X74808.0  -s 192.168.1.0/24   -j RETURN
    $IPTABLES -N GOOD_GUYS_0_3
    $IPTABLES -A Cid40710X74808.0  -j GOOD_GUYS_0_3
    $IPTABLES -A GOOD_GUYS_0_3  -j LOG  --log-level debug
    $IPTABLES -A GOOD_GUYS_0_3  -j DROP
    # ================ Table 'filter', rule set Policy
    # 
    # Rule 0 (eth0)
    # 
    echo "Rule 0 (eth0)"
    # 
    $IPTABLES -N Cid3C5987DC.1
    $IPTABLES -A INPUT -i eth0   -s 22.22.22.22   -j Cid3C5987DC.1
    $IPTABLES -N Cid3C5987DC.0
    $IPTABLES -A Cid3C5987DC.1 -p icmp  -j Cid3C5987DC.0
    $IPTABLES -A Cid3C5987DC.1 -p 50  -j Cid3C5987DC.0
    $IPTABLES -N Cid3C5987DC.2
    $IPTABLES -A INPUT -i eth0   -s 192.168.1.1   -j Cid3C5987DC.2
    $IPTABLES -A Cid3C5987DC.2 -p icmp  -j Cid3C5987DC.0
    $IPTABLES -A Cid3C5987DC.2 -p 50  -j Cid3C5987DC.0
    $IPTABLES -N Cid3C5987DC.3
    $IPTABLES -A FORWARD -i eth0   -s 22.22.22.22   -j Cid3C5987DC.3
    $IPTABLES -A Cid3C5987DC.3 -p icmp  -j Cid3C5987DC.0
    $IPTABLES -A Cid3C5987DC.3 -p 50  -j Cid3C5987DC.0
    $IPTABLES -N Cid3C5987DC.4
    $IPTABLES -A FORWARD -i eth0   -s 192.168.1.1   -j Cid3C5987DC.4
    $IPTABLES -A Cid3C5987DC.4 -p icmp  -j Cid3C5987DC.0
    $IPTABLES -A Cid3C5987DC.4 -p 50  -j Cid3C5987DC.0
    $IPTABLES -A Cid3C5987DC.0  -d 22.22.22.22   -j RETURN
    $IPTABLES -A Cid3C5987DC.0  -d 192.168.1.1   -j RETURN
    $IPTABLES -N In_RULE_0_3
    $IPTABLES -A Cid3C5987DC.0  -m hashlimit --hashlimit 1/hour --hashlimit-burst 2 --hashlimit-mode srcip,srcport --hashlimit-name htable_rule_0 -j In_RULE_0_3
    $IPTABLES -A In_RULE_0_3  -j LOG  --log-level debug
    $IPTABLES -A In_RULE_0_3  -j DROP
    $IPTABLES -N Cid3C5987DC.6
    $IPTABLES -A OUTPUT -o eth0   -s 22.22.22.22   -j Cid3C5987DC.6
    $IPTABLES -N Cid3C5987DC.5
    $IPTABLES -A Cid3C5987DC.6 -p icmp  -j Cid3C5987DC.5
    $IPTABLES -A Cid3C5987DC.6 -p 50  -j Cid3C5987DC.5
    $IPTABLES -N Cid3C5987DC.7
    $IPTABLES -A OUTPUT -o eth0   -s 192.168.1.1   -j Cid3C5987DC.7
    $IPTABLES -A Cid3C5987DC.7 -p icmp  -j Cid3C5987DC.5
    $IPTABLES -A Cid3C5987DC.7 -p 50  -j Cid3C5987DC.5
    $IPTABLES -A Cid3C5987DC.5  -d 22.22.22.22   -j RETURN
    $IPTABLES -A Cid3C5987DC.5  -d 192.168.1.1   -j RETURN
    $IPTABLES -N Out_RULE_0_3
    $IPTABLES -A Cid3C5987DC.5  -m hashlimit --hashlimit 1/hour --hashlimit-burst 2 --hashlimit-mode srcip,srcport --hashlimit-name htable_rule_0 -j Out_RULE_0_3
    $IPTABLES -A Out_RULE_0_3  -j LOG  --log-level debug
    $IPTABLES -A Out_RULE_0_3  -j DROP
    # 
    # Rule 1 (eth0)
    # 
    echo "Rule 1 (eth0)"
    # 
    $IPTABLES -N Cid3CD34BEF.1
    $IPTABLES -A INPUT -i eth0  -p icmp  -j Cid3CD34BEF.1
    $IPTABLES -A INPUT -i eth0  -p 50  -j Cid3CD34BEF.1
    $IPTABLES -N Cid3CD34BEF.0
    $IPTABLES -A Cid3CD34BEF.1  -s 192.168.1.10   -j Cid3CD34BEF.0
    $IPTABLES -A Cid3CD34BEF.1  -s 192.168.1.20   -j Cid3CD34BEF.0
    $IPTABLES -N Cid3CD34BEF.2
    $IPTABLES -A FORWARD -i eth0  -p icmp  -j Cid3CD34BEF.2
    $IPTABLES -A FORWARD -i eth0  -p 50  -j Cid3CD34BEF.2
    $IPTABLES -A Cid3CD34BEF.2  -s 192.168.1.10   -j Cid3CD34BEF.0
    $IPTABLES -A Cid3CD34BEF.2  -s 192.168.1.20   -j Cid3CD34BEF.0
    $IPTABLES -A Cid3CD34BEF.0  -d 192.168.1.10   -j RETURN
    $IPTABLES -A Cid3CD34BEF.0  -d 192.168.1.20   -j RETURN
    $IPTABLES -A Cid3CD34BEF.0  -m hashlimit --hashlimit 1/hour --hashlimit-burst 2 --hashlimit-mode dstip,dstport --hashlimit-name htable_rule_1 -j DROP
    $IPTABLES -N Cid3CD34BEF.4
    $IPTABLES -A FORWARD -o eth0  -p icmp  -j Cid3CD34BEF.4
    $IPTABLES -A FORWARD -o eth0  -p 50  -j Cid3CD34BEF.4
    $IPTABLES -N Cid3CD34BEF.3
    $IPTABLES -A Cid3CD34BEF.4  -s 192.168.1.10   -j Cid3CD34BEF.3
    $IPTABLES -A Cid3CD34BEF.4  -s 192.168.1.20   -j Cid3CD34BEF.3
    $IPTABLES -A Cid3CD34BEF.3  -d 192.168.1.10   -j RETURN
    $IPTABLES -A Cid3CD34BEF.3  -d 192.168.1.20   -j RETURN
    $IPTABLES -A Cid3CD34BEF.3  -m hashlimit --hashlimit 1/hour --hashlimit-burst 2 --hashlimit-mode dstip,dstport --hashlimit-name htable_rule_1 -j DROP
    # 
    # Rule 2 (eth1)
    # 
    echo "Rule 2 (eth1)"
    # 
    # Anti-spoofing rule
    $IPTABLES -N In_RULE_2
    $IPTABLES -A INPUT -i eth1   -s 22.22.22.22   -j In_RULE_2
    $IPTABLES -A INPUT -i eth1   -s 22.22.23.23   -j In_RULE_2
    $IPTABLES -A INPUT -i eth1   -s 192.168.1.1   -j In_RULE_2
    $IPTABLES -A INPUT -i eth1   -s 192.168.2.1   -j In_RULE_2
    $IPTABLES -A INPUT -i eth1   -s 192.168.1.0/24   -j In_RULE_2
    $IPTABLES -A FORWARD -i eth1   -s 22.22.22.22   -j In_RULE_2
    $IPTABLES -A FORWARD -i eth1   -s 22.22.23.23   -j In_RULE_2
    $IPTABLES -A FORWARD -i eth1   -s 192.168.1.1   -j In_RULE_2
    $IPTABLES -A FORWARD -i eth1   -s 192.168.2.1   -j In_RULE_2
    $IPTABLES -A FORWARD -i eth1   -s 192.168.1.0/24   -j In_RULE_2
    $IPTABLES -A In_RULE_2  -j LOG  --log-level debug
    $IPTABLES -A In_RULE_2  -j DROP
    # 
    # Rule 3 (eth1)
    # 
    echo "Rule 3 (eth1)"
    # 
    # Anti-spoofing rule
    $IPTABLES -N Out_RULE_3
    $IPTABLES -A OUTPUT -o eth1   -s ! 192.168.1.0/24   -j Out_RULE_3
    $IPTABLES -A FORWARD -o eth1   -s ! 192.168.1.0/24   -j Out_RULE_3
    $IPTABLES -A Out_RULE_3  -j LOG  --log-level debug
    $IPTABLES -A Out_RULE_3  -j DROP
    # 
    # Rule 4 (eth1)
    # 
    echo "Rule 4 (eth1)"
    # 
    # Anti-spoofing rule
    $IPTABLES -N Cid40DBCD36.0
    $IPTABLES -A OUTPUT -o eth1   -j Cid40DBCD36.0
    $IPTABLES -A Cid40DBCD36.0  -s 22.22.22.22   -j RETURN
    $IPTABLES -A Cid40DBCD36.0  -s 22.22.23.23   -j RETURN
    $IPTABLES -A Cid40DBCD36.0  -s 192.168.1.1   -j RETURN
    $IPTABLES -A Cid40DBCD36.0  -s 192.168.2.1   -j RETURN
    $IPTABLES -N Out_RULE_4_3
    $IPTABLES -A Cid40DBCD36.0  -j Out_RULE_4_3
    $IPTABLES -A Out_RULE_4_3  -j LOG  --log-level debug
    $IPTABLES -A Out_RULE_4_3  -j DROP
    $IPTABLES -N Cid40DBCD36.1
    $IPTABLES -A FORWARD -o eth1   -j Cid40DBCD36.1
    $IPTABLES -A Cid40DBCD36.1  -s 192.168.1.0/24   -j RETURN
    $IPTABLES -A Cid40DBCD36.1  -j Out_RULE_4_3
    # 
    # Rule 5 (eth2)
    # 
    echo "Rule 5 (eth2)"
    # 
    $IPTABLES -A INPUT -i eth2   -s 192.168.2.0/24   -m state --state NEW  -j ACCEPT
    $IPTABLES -A FORWARD -i eth2   -s 192.168.2.0/24   -m state --state NEW  -j ACCEPT
    $IPTABLES -A OUTPUT -o eth2   -s 192.168.2.0/24   -m state --state NEW  -j ACCEPT
    $IPTABLES -A FORWARD -o eth2   -s 192.168.2.0/24   -m state --state NEW  -j ACCEPT
    # 
    # Rule 6 (eth2)
    # 
    echo "Rule 6 (eth2)"
    # 
    $IPTABLES -N In_RULE_6
    $IPTABLES -A INPUT -i ! eth2   -s 192.168.2.0/24   -j In_RULE_6
    $IPTABLES -A FORWARD -i ! eth2   -s 192.168.2.0/24   -j In_RULE_6
    $IPTABLES -A In_RULE_6  -j LOG  --log-level debug
    $IPTABLES -A In_RULE_6  -j DROP
    # 
    # Rule 7 (eth1,eth3)
    # 
    echo "Rule 7 (eth1,eth3)"
    # 
    $IPTABLES -N In_RULE_7
    $IPTABLES -A INPUT -i eth0   -s 22.22.23.128/25   -j In_RULE_7
    $IPTABLES -A INPUT -i eth0   -s 33.33.33.0/24   -j In_RULE_7
    $IPTABLES -A INPUT -i eth2   -s 22.22.23.128/25   -j In_RULE_7
    $IPTABLES -A INPUT -i eth2   -s 33.33.33.0/24   -j In_RULE_7
    $IPTABLES -A FORWARD -i eth0   -s 22.22.23.128/25   -j In_RULE_7
    $IPTABLES -A FORWARD -i eth0   -s 33.33.33.0/24   -j In_RULE_7
    $IPTABLES -A FORWARD -i eth2   -s 22.22.23.128/25   -j In_RULE_7
    $IPTABLES -A FORWARD -i eth2   -s 33.33.33.0/24   -j In_RULE_7
    $IPTABLES -A In_RULE_7  -j LOG  --log-level debug
    $IPTABLES -A In_RULE_7  -j DROP
    # 
    # Rule 8 (lo)
    # 
    echo "Rule 8 (lo)"
    # 
    $IPTABLES -A INPUT -i lo   -m state --state NEW  -j ACCEPT
    $IPTABLES -A OUTPUT -o lo   -m state --state NEW  -j ACCEPT
    # 
    # Rule 9 (eth0,eth2)
    # 
    echo "Rule 9 (eth0,eth2)"
    # 
    $IPTABLES -N Cid433D045026912.0
    $IPTABLES -A INPUT -i eth0   -j Cid433D045026912.0
    $IPTABLES -A INPUT -i eth2   -j Cid433D045026912.0
    $IPTABLES -A FORWARD -i eth0   -j Cid433D045026912.0
    $IPTABLES -A FORWARD -i eth2   -j Cid433D045026912.0
    $IPTABLES -A Cid433D045026912.0  -s 192.168.1.0/24   -j RETURN
    $IPTABLES -A Cid433D045026912.0  -s 192.168.2.0/24   -j RETURN
    $IPTABLES -N In_RULE_9_3
    $IPTABLES -A Cid433D045026912.0  -j In_RULE_9_3
    $IPTABLES -A In_RULE_9_3  -j LOG  --log-level debug
    $IPTABLES -A In_RULE_9_3  -j DROP
    # 
    # Rule 10 (eth1,eth3)
    # 
    echo "Rule 10 (eth1,eth3)"
    # 
    $IPTABLES -N Cid434D389E26912.0
    $IPTABLES -A INPUT -i eth1   -m state --state NEW  -j Cid434D389E26912.0
    $IPTABLES -A INPUT -i eth3   -m state --state NEW  -j Cid434D389E26912.0
    $IPTABLES -A FORWARD -i eth1   -m state --state NEW  -j Cid434D389E26912.0
    $IPTABLES -A FORWARD -i eth3   -m state --state NEW  -j Cid434D389E26912.0
    $IPTABLES -A Cid434D389E26912.0  -s 22.22.23.128/25   -j RETURN
    $IPTABLES -A Cid434D389E26912.0  -s 33.33.33.0/24   -j RETURN
    $IPTABLES -A Cid434D389E26912.0  -j ACCEPT
    # 
    # Rule 11 (global)
    # 
    echo "Rule 11 (global)"
    # 
    $IPTABLES -N RULE_11
    $IPTABLES -A RULE_11  -j RETURN
    $IPTABLES -A OUTPUT  -j RULE_11
    $IPTABLES -A INPUT  -j RULE_11
    $IPTABLES -A FORWARD  -j RULE_11
    # 
    # Rule 12 (global)
    # 
    echo "Rule 12 (global)"
    # 
    $IPTABLES -N RULE_12
    $IPTABLES -A OUTPUT -p tcp -m tcp   --tcp-flags SYN,RST,ACK SYN   -j RULE_12
    $IPTABLES -A INPUT -p tcp -m tcp   --tcp-flags SYN,RST,ACK SYN   -j RULE_12
    $IPTABLES -A FORWARD -p tcp -m tcp   --tcp-flags SYN,RST,ACK SYN   -j RULE_12
    $IPTABLES -A RULE_12  -j LOG  --log-level debug
    $IPTABLES -A RULE_12  -j DROP
    # 
    # Rule 13 (global)
    # 
    echo "Rule 13 (global)"
    # 
    $IPTABLES -N Cid3B9AB902.0
    $IPTABLES -A OUTPUT  -j Cid3B9AB902.0
    $IPTABLES -A INPUT  -j Cid3B9AB902.0
    $IPTABLES -A FORWARD  -j Cid3B9AB902.0
    $IPTABLES -A Cid3B9AB902.0 -p tcp -m tcp   --tcp-flags SYN,RST,ACK SYN   -j RETURN
    $IPTABLES -N RULE_13_3
    $IPTABLES -A Cid3B9AB902.0  -j RULE_13_3
    $IPTABLES -A RULE_13_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_13_3  -j DROP
    # 
    # Rule 14 (global)
    # 
    echo "Rule 14 (global)"
    # 
    # hostF has the same IP address as firewal.
    $IPTABLES -N RULE_14
    $IPTABLES -A OUTPUT -p icmp  -m icmp  -d 192.168.1.1   --icmp-type 8/0   -m state --state NEW  -j RULE_14
    $IPTABLES -A INPUT -p icmp  -m icmp  -d 192.168.1.1   --icmp-type 8/0   -m state --state NEW  -j RULE_14
    $IPTABLES -A RULE_14  -j LOG  --log-level debug
    $IPTABLES -A RULE_14  -j ACCEPT
    # 
    # Rule 15 (global)
    # 
    echo "Rule 15 (global)"
    # 
    $IPTABLES -N Cid434B03D526912.0
    $IPTABLES -A OUTPUT  -m state --state NEW  -j Cid434B03D526912.0
    $IPTABLES -A INPUT  -m state --state NEW  -j Cid434B03D526912.0
    $IPTABLES -A FORWARD  -m state --state NEW  -j Cid434B03D526912.0
    $IPTABLES -A Cid434B03D526912.0  -s 192.168.1.0/24   -j RETURN
    $IPTABLES -A Cid434B03D526912.0  -s 192.168.2.0/24   -j RETURN
    $IPTABLES -A Cid434B03D526912.0  -j ACCEPT
    # 
    # Rule 16 (global)
    # 
    echo "Rule 16 (global)"
    # 
    # testing negation in the policy rule
    $IPTABLES -N Cid3B021E10.0
    $IPTABLES -A OUTPUT -p icmp  -m icmp  --icmp-type 3  -j Cid3B021E10.0
    $IPTABLES -A INPUT -p icmp  -m icmp  --icmp-type 3  -j Cid3B021E10.0
    $IPTABLES -A FORWARD -p icmp  -m icmp  --icmp-type 3  -j Cid3B021E10.0
    $IPTABLES -A Cid3B021E10.0  -s 192.168.1.10   -j RETURN
    $IPTABLES -A Cid3B021E10.0  -s 192.168.1.20   -j RETURN
    $IPTABLES -N RULE_16_3
    $IPTABLES -A Cid3B021E10.0  -m limit --limit 10/minute -j RULE_16_3
    $IPTABLES -A RULE_16_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_16_3  -j DROP
    # 
    # Rule 17 (global)
    # 
    echo "Rule 17 (global)"
    # 
    # testing negation in the policy rule
    $IPTABLES -N Cid40C0D096.0
    $IPTABLES -A OUTPUT -p tcp -m tcp  -m multiport  --dports 80,443  -j Cid40C0D096.0
    $IPTABLES -A INPUT -p tcp -m tcp  -m multiport  --dports 80,443  -j Cid40C0D096.0
    $IPTABLES -A FORWARD -p tcp -m tcp  -m multiport  --dports 80,443  -j Cid40C0D096.0
    $IPTABLES -A Cid40C0D096.0  -s 192.168.1.10   -j RETURN
    $IPTABLES -A Cid40C0D096.0  -s 192.168.1.20   -j RETURN
    $IPTABLES -N RULE_17_3
    $IPTABLES -A Cid40C0D096.0  -m limit --limit 10/minute -j RULE_17_3
    $IPTABLES -A RULE_17_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_17_3  -j RETURN
    # 
    # Rule 18 (global)
    # 
    echo "Rule 18 (global)"
    # 
    # testing negation in the policy rule
    $IPTABLES -N Cid40C0D10A.0
    $IPTABLES -A OUTPUT -p tcp -m tcp  -m multiport  --dports 80,443  -m state --state NEW  -j Cid40C0D10A.0
    $IPTABLES -A INPUT -p tcp -m tcp  -m multiport  --dports 80,443  -m state --state NEW  -j Cid40C0D10A.0
    $IPTABLES -A FORWARD -p tcp -m tcp  -m multiport  --dports 80,443  -m state --state NEW  -j Cid40C0D10A.0
    $IPTABLES -A Cid40C0D10A.0  -s 192.168.1.10   -j RETURN
    $IPTABLES -A Cid40C0D10A.0  -s 192.168.1.20   -j RETURN
    $IPTABLES -N RULE_18_3
    $IPTABLES -A Cid40C0D10A.0  -m limit --limit 10/minute -j RULE_18_3
    $IPTABLES -A RULE_18_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_18_3  -j ACCEPT
    # 
    # Rule 19 (global)
    # 
    echo "Rule 19 (global)"
    # 
    $IPTABLES -N Cid3B0B4A13.1
    $IPTABLES -A OUTPUT -p icmp  -m icmp  --icmp-type 3  -j Cid3B0B4A13.1
    $IPTABLES -N Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.1  -d 22.22.22.22   -j Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.1  -d 22.22.23.23   -j Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.1  -d 192.168.1.1   -j Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.1  -d 192.168.2.1   -j Cid3B0B4A13.0
    $IPTABLES -N Cid3B0B4A13.2
    $IPTABLES -A INPUT -p icmp  -m icmp  --icmp-type 3  -j Cid3B0B4A13.2
    $IPTABLES -A Cid3B0B4A13.2  -d 22.22.22.22   -j Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.2  -d 22.22.23.23   -j Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.2  -d 192.168.1.1   -j Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.2  -d 192.168.2.1   -j Cid3B0B4A13.0
    $IPTABLES -A Cid3B0B4A13.0  -s 192.168.1.10   -j RETURN
    $IPTABLES -A Cid3B0B4A13.0  -s 192.168.1.20   -j RETURN
    $IPTABLES -N RULE_19_3
    $IPTABLES -A Cid3B0B4A13.0  -j RULE_19_3
    $IPTABLES -A RULE_19_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_19_3  -j DROP
    # 
    # Rule 20 (global)
    # 
    echo "Rule 20 (global)"
    # 
    $IPTABLES -N Cid3B5535B7.0
    $IPTABLES -A OUTPUT  -d 192.168.1.0/24   -j Cid3B5535B7.0
    $IPTABLES -A Cid3B5535B7.0  -s 22.22.22.22   -j RETURN
    $IPTABLES -A Cid3B5535B7.0  -s 22.22.23.23   -j RETURN
    $IPTABLES -A Cid3B5535B7.0  -s 192.168.1.1   -j RETURN
    $IPTABLES -A Cid3B5535B7.0  -s 192.168.2.1   -j RETURN
    $IPTABLES -N Out_RULE_20_3
    $IPTABLES -A Cid3B5535B7.0  -j Out_RULE_20_3
    $IPTABLES -A Out_RULE_20_3  -j LOG  --log-level debug
    $IPTABLES -A Out_RULE_20_3  -j DROP
    $IPTABLES -N Cid3B5535B7.1
    $IPTABLES -A INPUT  -d 192.168.1.0/24   -j Cid3B5535B7.1
    $IPTABLES -A FORWARD  -d 192.168.1.0/24   -j Cid3B5535B7.1
    $IPTABLES -A Cid3B5535B7.1  -s 192.168.2.0/24   -j RETURN
    $IPTABLES -N RULE_20_3
    $IPTABLES -A Cid3B5535B7.1  -j RULE_20_3
    $IPTABLES -A RULE_20_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_20_3  -j DROP
    # 
    # Rule 21 (global)
    # 
    echo "Rule 21 (global)"
    # 
    $IPTABLES -N Cid40F1D905.0
    $IPTABLES -A OUTPUT  -d 192.168.1.0/24   -j Cid40F1D905.0
    $IPTABLES -A Cid40F1D905.0  -s 192.168.1.1   -j RETURN
    $IPTABLES -N Out_RULE_21_3
    $IPTABLES -A Cid40F1D905.0  -j Out_RULE_21_3
    $IPTABLES -A Out_RULE_21_3  -j LOG  --log-level debug
    $IPTABLES -A Out_RULE_21_3  -j DROP
    $IPTABLES -N Cid40F1D905.1
    $IPTABLES -A INPUT  -d 192.168.1.0/24   -j Cid40F1D905.1
    $IPTABLES -A FORWARD  -d 192.168.1.0/24   -j Cid40F1D905.1
    $IPTABLES -A Cid40F1D905.1  -s 192.168.2.0/24   -j RETURN
    $IPTABLES -N RULE_21_3
    $IPTABLES -A Cid40F1D905.1  -j RULE_21_3
    $IPTABLES -A RULE_21_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_21_3  -j DROP
    # 
    # Rule 22 (global)
    # 
    echo "Rule 22 (global)"
    # 
    $IPTABLES -N Cid3E74DF71.0
    $IPTABLES -A INPUT  -s 222.222.222.40   -j Cid3E74DF71.0
    $IPTABLES -A INPUT  -s 222.222.222.41   -j Cid3E74DF71.0
    $IPTABLES -A FORWARD  -s 222.222.222.40   -j Cid3E74DF71.0
    $IPTABLES -A FORWARD  -s 222.222.222.41   -j Cid3E74DF71.0
    $IPTABLES -A Cid3E74DF71.0  -d 192.168.1.10   -j RETURN
    $IPTABLES -A Cid3E74DF71.0  -d 192.168.1.20   -j RETURN
    $IPTABLES -N RULE_22_3
    $IPTABLES -A Cid3E74DF71.0  -j RULE_22_3
    $IPTABLES -A RULE_22_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_22_3  -j DROP
    # 
    # Rule 23 (global)
    # 
    echo "Rule 23 (global)"
    # 
    $IPTABLES -N Cid3B11F63D.0
    $IPTABLES -A INPUT  -s 192.168.1.0/24   -j Cid3B11F63D.0
    $IPTABLES -A INPUT  -s 192.168.2.0/24   -j Cid3B11F63D.0
    $IPTABLES -A OUTPUT  -s 192.168.1.0/24   -j Cid3B11F63D.0
    $IPTABLES -A OUTPUT  -s 192.168.2.0/24   -j Cid3B11F63D.0
    $IPTABLES -A FORWARD  -s 192.168.1.0/24   -j Cid3B11F63D.0
    $IPTABLES -A FORWARD  -s 192.168.2.0/24   -j Cid3B11F63D.0
    $IPTABLES -A Cid3B11F63D.0  -d 192.168.1.10   -j RETURN
    $IPTABLES -A Cid3B11F63D.0  -d 192.168.1.20   -j RETURN
    $IPTABLES -N RULE_23_3
    $IPTABLES -A Cid3B11F63D.0  -j RULE_23_3
    $IPTABLES -A RULE_23_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_23_3  -j DROP
    # 
    # Rule 24 (global)
    # 
    echo "Rule 24 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid3B021E6F.0
    $IPTABLES -A OUTPUT  -d 192.168.1.10   -j Cid3B021E6F.0
    $IPTABLES -A OUTPUT  -d 192.168.1.20   -j Cid3B021E6F.0
    $IPTABLES -A FORWARD  -d 192.168.1.10   -j Cid3B021E6F.0
    $IPTABLES -A FORWARD  -d 192.168.1.20   -j Cid3B021E6F.0
    $IPTABLES -A Cid3B021E6F.0 -p tcp -m tcp  -m multiport  --dports 25,22  -j RETURN
    $IPTABLES -N RULE_24_3
    $IPTABLES -A Cid3B021E6F.0  -j RULE_24_3
    $IPTABLES -A RULE_24_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_24_3  -j DROP
    # 
    # Rule 25 (global)
    # 
    echo "Rule 25 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid3CCA2CF4.0
    $IPTABLES -A OUTPUT  -d 192.168.1.10   -m state --state NEW  -j Cid3CCA2CF4.0
    $IPTABLES -A OUTPUT  -d 192.168.1.20   -m state --state NEW  -j Cid3CCA2CF4.0
    $IPTABLES -A FORWARD  -d 192.168.1.10   -m state --state NEW  -j Cid3CCA2CF4.0
    $IPTABLES -A FORWARD  -d 192.168.1.20   -m state --state NEW  -j Cid3CCA2CF4.0
    $IPTABLES -A Cid3CCA2CF4.0 -p tcp -m tcp  -m multiport  --dports 25,22  -j RETURN
    $IPTABLES -N RULE_25_3
    $IPTABLES -A Cid3CCA2CF4.0  -j RULE_25_3
    $IPTABLES -A RULE_25_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_25_3  -j ACCEPT
    # 
    # Rule 26 (global)
    # 
    echo "Rule 26 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid3EA925F1.0
    $IPTABLES -A OUTPUT  -d 192.168.1.10   -m state --state NEW  -j Cid3EA925F1.0
    $IPTABLES -A OUTPUT  -d 192.168.1.20   -m state --state NEW  -j Cid3EA925F1.0
    $IPTABLES -A FORWARD  -d 192.168.1.10   -m state --state NEW  -j Cid3EA925F1.0
    $IPTABLES -A FORWARD  -d 192.168.1.20   -m state --state NEW  -j Cid3EA925F1.0
    $IPTABLES -A Cid3EA925F1.0 -p tcp -m tcp  --dport 25  -j RETURN
    $IPTABLES -N RULE_26_3
    $IPTABLES -A Cid3EA925F1.0  -j RULE_26_3
    $IPTABLES -A RULE_26_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_26_3  -j ACCEPT
    # 
    # Rule 27 (global)
    # 
    echo "Rule 27 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid3EA9225C.0
    $IPTABLES -A OUTPUT  -d 192.168.1.10   -m state --state NEW  -j Cid3EA9225C.0
    $IPTABLES -A OUTPUT  -d 192.168.1.20   -m state --state NEW  -j Cid3EA9225C.0
    $IPTABLES -A FORWARD  -d 192.168.1.10   -m state --state NEW  -j Cid3EA9225C.0
    $IPTABLES -A FORWARD  -d 192.168.1.20   -m state --state NEW  -j Cid3EA9225C.0
    $IPTABLES -A Cid3EA9225C.0 -p icmp  -m icmp  --icmp-type any  -j RETURN
    $IPTABLES -N RULE_27_3
    $IPTABLES -A Cid3EA9225C.0  -j RULE_27_3
    $IPTABLES -A RULE_27_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_27_3  -j ACCEPT
    # 
    # Rule 28 (global)
    # 
    echo "Rule 28 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid4144E299.1
    $IPTABLES -A OUTPUT  -m state --state NEW  -j Cid4144E299.1
    $IPTABLES -A INPUT  -m state --state NEW  -j Cid4144E299.1
    $IPTABLES -A FORWARD  -m state --state NEW  -j Cid4144E299.1
    $IPTABLES -A Cid4144E299.1  -d 192.168.1.10   -j RETURN
    $IPTABLES -A Cid4144E299.1  -d 192.168.1.20   -j RETURN
    $IPTABLES -N Cid4144E299.0
    $IPTABLES -A Cid4144E299.1  -j Cid4144E299.0
    $IPTABLES -A Cid4144E299.0 -p icmp  -m icmp  --icmp-type any  -j RETURN
    $IPTABLES -A Cid4144E299.0  -j ACCEPT
    # 
    # Rule 29 (global)
    # 
    echo "Rule 29 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid41449248.1
    $IPTABLES -A OUTPUT  -m state --state NEW -m time  --timestart 09:00  --timestop 17:00  --days Mon,Tue,Wed,Thu,Fri -j Cid41449248.1
    $IPTABLES -N Cid41449248.0
    $IPTABLES -A Cid41449248.1  -d 192.168.1.10   -j Cid41449248.0
    $IPTABLES -A Cid41449248.1  -d 192.168.1.20   -j Cid41449248.0
    $IPTABLES -N Cid41449248.2
    $IPTABLES -A FORWARD  -m state --state NEW -m time  --timestart 09:00  --timestop 17:00  --days Mon,Tue,Wed,Thu,Fri -j Cid41449248.2
    $IPTABLES -A Cid41449248.2  -d 192.168.1.10   -j Cid41449248.0
    $IPTABLES -A Cid41449248.2  -d 192.168.1.20   -j Cid41449248.0
    $IPTABLES -A Cid41449248.0 -p tcp -m tcp  --dport 80  -j RETURN
    $IPTABLES -A Cid41449248.0  -j ACCEPT
    # 
    # Rule 30 (global)
    # 
    echo "Rule 30 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid414532F3.1
    $IPTABLES -A OUTPUT -p tcp -m tcp  --dport 80  -m state --state NEW  -j Cid414532F3.1
    $IPTABLES -A INPUT -p tcp -m tcp  --dport 80  -m state --state NEW  -j Cid414532F3.1
    $IPTABLES -A FORWARD -p tcp -m tcp  --dport 80  -m state --state NEW  -j Cid414532F3.1
    $IPTABLES -A Cid414532F3.1 -m time  --timestart 09:00  --timestop 17:00  --days Mon,Tue,Wed,Thu,Fri -j RETURN
    $IPTABLES -N Cid414532F3.0
    $IPTABLES -A Cid414532F3.1  -j Cid414532F3.0
    $IPTABLES -A Cid414532F3.0  -d 192.168.1.10   -j RETURN
    $IPTABLES -A Cid414532F3.0  -d 192.168.1.20   -j RETURN
    $IPTABLES -A Cid414532F3.0  -j ACCEPT
    # 
    # Rule 31 (global)
    # 
    echo "Rule 31 (global)"
    # 
    # testing negation in service field
    $IPTABLES -N Cid41449257.1
    $IPTABLES -A OUTPUT  -d 192.168.1.10   -m state --state NEW  -j Cid41449257.1
    $IPTABLES -A OUTPUT  -d 192.168.1.20   -m state --state NEW  -j Cid41449257.1
    $IPTABLES -A FORWARD  -d 192.168.1.10   -m state --state NEW  -j Cid41449257.1
    $IPTABLES -A FORWARD  -d 192.168.1.20   -m state --state NEW  -j Cid41449257.1
    $IPTABLES -A Cid41449257.1 -m time  --timestart 09:00  --timestop 17:00  --days Mon,Tue,Wed,Thu,Fri -j RETURN
    $IPTABLES -N Cid41449257.0
    $IPTABLES -A Cid41449257.1  -j Cid41449257.0
    $IPTABLES -A Cid41449257.0 -p tcp -m tcp  --dport 80  -j RETURN
    $IPTABLES -A Cid41449257.0  -j ACCEPT
    # 
    # Rule 32 (global)
    # 
    echo "Rule 32 (global)"
    # 
    $IPTABLES -N Cid4368F08A15884.1
    $IPTABLES -A INPUT -p tcp -m tcp  --dport 80  -m state --state NEW  -j Cid4368F08A15884.1
    $IPTABLES -N Cid4368F08A15884.0
    $IPTABLES -A Cid4368F08A15884.1  -s 22.22.22.22   -j Cid4368F08A15884.0
    $IPTABLES -A Cid4368F08A15884.1  -s 22.22.23.23   -j Cid4368F08A15884.0
    $IPTABLES -A Cid4368F08A15884.1  -s 192.168.1.1   -j Cid4368F08A15884.0
    $IPTABLES -A Cid4368F08A15884.1  -s 192.168.2.1   -j Cid4368F08A15884.0
    $IPTABLES -A Cid4368F08A15884.0  -d 22.22.22.22   -j RETURN
    $IPTABLES -A Cid4368F08A15884.0  -d 22.22.23.23   -j RETURN
    $IPTABLES -A Cid4368F08A15884.0  -d 192.168.1.1   -j RETURN
    $IPTABLES -A Cid4368F08A15884.0  -d 192.168.2.1   -j RETURN
    $IPTABLES -A Cid4368F08A15884.0  -j ACCEPT
    $IPTABLES -N Cid4368F08A15884.2
    $IPTABLES -A OUTPUT -p tcp -m tcp  --dport 80  -m state --state NEW  -j Cid4368F08A15884.2
    $IPTABLES -A Cid4368F08A15884.2  -s 22.22.22.22   -j ACCEPT
    $IPTABLES -A Cid4368F08A15884.2  -s 22.22.23.23   -j ACCEPT
    $IPTABLES -A Cid4368F08A15884.2  -s 192.168.1.1   -j ACCEPT
    $IPTABLES -A Cid4368F08A15884.2  -s 192.168.2.1   -j ACCEPT
    # 
    # Rule 33 (global)
    # 
    echo "Rule 33 (global)"
    # 
    $IPTABLES -N Cid3E74D8BB.1
    $IPTABLES -A INPUT -p tcp -m tcp  --dport 22  -m state --state NEW  -j Cid3E74D8BB.1
    $IPTABLES -N Cid3E74D8BB.0
    $IPTABLES -A Cid3E74D8BB.1  -s 22.22.22.22   -j Cid3E74D8BB.0
    $IPTABLES -A Cid3E74D8BB.1  -s 22.22.23.23   -j Cid3E74D8BB.0
    $IPTABLES -A Cid3E74D8BB.1  -s 192.168.1.1   -j Cid3E74D8BB.0
    $IPTABLES -A Cid3E74D8BB.1  -s 192.168.2.1   -j Cid3E74D8BB.0
    $IPTABLES -A INPUT -p tcp -m tcp  -s 192.168.2.0/24   --dport 22  -m state --state NEW  -j Cid3E74D8BB.0
    $IPTABLES -A Cid3E74D8BB.0  -d 22.22.22.22   -j RETURN
    $IPTABLES -A Cid3E74D8BB.0  -d 22.22.23.23   -j RETURN
    $IPTABLES -A Cid3E74D8BB.0  -d 192.168.1.1   -j RETURN
    $IPTABLES -A Cid3E74D8BB.0  -d 192.168.2.1   -j RETURN
    $IPTABLES -A Cid3E74D8BB.0  -j ACCEPT
    $IPTABLES -N Cid3E74D8BB.3
    $IPTABLES -A OUTPUT -p tcp -m tcp  --dport 22  -m state --state NEW  -j Cid3E74D8BB.3
    $IPTABLES -N Cid3E74D8BB.2
    $IPTABLES -A Cid3E74D8BB.3  -s 22.22.22.22   -j Cid3E74D8BB.2
    $IPTABLES -A Cid3E74D8BB.3  -s 22.22.23.23   -j Cid3E74D8BB.2
    $IPTABLES -A Cid3E74D8BB.3  -s 192.168.1.1   -j Cid3E74D8BB.2
    $IPTABLES -A Cid3E74D8BB.3  -s 192.168.2.1   -j Cid3E74D8BB.2
    $IPTABLES -A OUTPUT -p tcp -m tcp  -s 192.168.2.0/24   --dport 22  -m state --state NEW  -j Cid3E74D8BB.2
    $IPTABLES -A FORWARD -p tcp -m tcp  -s 192.168.2.0/24   --dport 22  -m state --state NEW  -j Cid3E74D8BB.2
    $IPTABLES -A Cid3E74D8BB.2  -d 192.168.1.0/24   -j RETURN
    $IPTABLES -A Cid3E74D8BB.2  -j ACCEPT
    # 
    # Rule 34 (global)
    # 
    echo "Rule 34 (global)"
    # 
    $IPTABLES -N Cid3B45739A.1
    $IPTABLES -A INPUT  -s 22.22.22.22   -j Cid3B45739A.1
    $IPTABLES -N Cid3B45739A.0
    $IPTABLES -A Cid3B45739A.1 -p icmp  -j Cid3B45739A.0
    $IPTABLES -A Cid3B45739A.1 -p 50  -j Cid3B45739A.0
    $IPTABLES -N Cid3B45739A.2
    $IPTABLES -A INPUT  -s 192.168.1.1   -j Cid3B45739A.2
    $IPTABLES -A Cid3B45739A.2 -p icmp  -j Cid3B45739A.0
    $IPTABLES -A Cid3B45739A.2 -p 50  -j Cid3B45739A.0
    $IPTABLES -N Cid3B45739A.3
    $IPTABLES -A OUTPUT  -s 22.22.22.22   -j Cid3B45739A.3
    $IPTABLES -A Cid3B45739A.3 -p icmp  -j Cid3B45739A.0
    $IPTABLES -A Cid3B45739A.3 -p 50  -j Cid3B45739A.0
    $IPTABLES -N Cid3B45739A.4
    $IPTABLES -A OUTPUT  -s 192.168.1.1   -j Cid3B45739A.4
    $IPTABLES -A Cid3B45739A.4 -p icmp  -j Cid3B45739A.0
    $IPTABLES -A Cid3B45739A.4 -p 50  -j Cid3B45739A.0
    $IPTABLES -A Cid3B45739A.0  -d 22.22.22.22   -j RETURN
    $IPTABLES -A Cid3B45739A.0  -d 192.168.1.1   -j RETURN
    $IPTABLES -N RULE_34_3
    $IPTABLES -A Cid3B45739A.0  -j RULE_34_3
    $IPTABLES -A RULE_34_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_34_3  -j DROP
    # 
    # Rule 35 (global)
    # 
    echo "Rule 35 (global)"
    # 
    # double negation rule
    $IPTABLES -N Cid4067B2C2.1
    $IPTABLES -A OUTPUT  -j Cid4067B2C2.1
    $IPTABLES -A INPUT  -j Cid4067B2C2.1
    $IPTABLES -A FORWARD  -j Cid4067B2C2.1
    $IPTABLES -A Cid4067B2C2.1  -d 192.168.1.10   -j RETURN
    $IPTABLES -A Cid4067B2C2.1  -d 192.168.1.20   -j RETURN
    $IPTABLES -N Cid4067B2C2.0
    $IPTABLES -A Cid4067B2C2.1  -j Cid4067B2C2.0
    $IPTABLES -A Cid4067B2C2.0 -p tcp -m tcp  -m multiport  --dports 3128,8080  -j RETURN
    $IPTABLES -N RULE_35_3
    $IPTABLES -A Cid4067B2C2.0  -j RULE_35_3
    $IPTABLES -A RULE_35_3  -j LOG  --log-level debug
    $IPTABLES -A RULE_35_3  -j DROP
    # 
    # Rule 36 (global)
    # 
    echo "Rule 36 (global)"
    # 
    $IPTABLES -N Cid41A88DF6.0
    $IPTABLES -A INPUT  -m state --state NEW  -j Cid41A88DF6.0
    $IPTABLES -A Cid41A88DF6.0  -d 192.168.1.1   -j RETURN
    $IPTABLES -A Cid41A88DF6.0  -d 192.168.2.1   -j RETURN
    $IPTABLES -A Cid41A88DF6.0  -j ACCEPT
    $IPTABLES -A OUTPUT  -m state --state NEW  -j ACCEPT
    $IPTABLES -A FORWARD  -m state --state NEW  -j ACCEPT
    # 
    # Rule 37 (global)
    # 
    echo "Rule 37 (global)"
    # 
    $IPTABLES -N Cid41B5176E.0
    $IPTABLES -A OUTPUT  -d 192.168.1.0/24   -m state --state NEW  -j Cid41B5176E.0
    $IPTABLES -A Cid41B5176E.0  -s 192.168.1.1   -j RETURN
    $IPTABLES -A Cid41B5176E.0  -s 192.168.2.1   -j RETURN
    $IPTABLES -A Cid41B5176E.0  -j ACCEPT
    $IPTABLES -A INPUT  -d 192.168.1.0/24   -m state --state NEW  -j ACCEPT
    $IPTABLES -A FORWARD  -d 192.168.1.0/24   -m state --state NEW  -j ACCEPT
    # 
    # Rule 38 (global)
    # 
    echo "Rule 38 (global)"
    # 
    $IPTABLES -N Cid4143BD3F.0
    $IPTABLES -A INPUT -p tcp -m tcp  -s 192.168.1.0/24   --dport 25  -m state --state NEW  -j Cid4143BD3F.0
    $IPTABLES -A OUTPUT -p tcp -m tcp  -s 192.168.1.0/24   --dport 25  -m state --state NEW  -j Cid4143BD3F.0
    $IPTABLES -A FORWARD -p tcp -m tcp  -s 192.168.1.0/24   --dport 25  -m state --state NEW  -j Cid4143BD3F.0
    $IPTABLES -A Cid4143BD3F.0 -m time  --timestart 00:00  --timestop 23:59  --days Sat -j RETURN
    $IPTABLES -A Cid4143BD3F.0 -m time  --timestart 00:00  --timestop 23:59  --days Sun -j RETURN
    $IPTABLES -A Cid4143BD3F.0  -j ACCEPT
    # 
    # Rule 39 (global)
    # 
    echo "Rule 39 (global)"
    # 
    $IPTABLES -N Cid4143BD1A.0
    $IPTABLES -A INPUT -p tcp -m tcp  -s 192.168.1.0/24   --dport 80  -m state --state NEW  -j Cid4143BD1A.0
    $IPTABLES -A OUTPUT -p tcp -m tcp  -s 192.168.1.0/24   --dport 80  -m state --state NEW  -j Cid4143BD1A.0
    $IPTABLES -A FORWARD -p tcp -m tcp  -s 192.168.1.0/24   --dport 80  -m state --state NEW  -j Cid4143BD1A.0
    $IPTABLES -A Cid4143BD1A.0 -m time  --timestart 09:00  --timestop 17:00  --days Mon,Tue,Wed,Thu,Fri -j RETURN
    $IPTABLES -A Cid4143BD1A.0  -j ACCEPT
    # 
    # Rule 40 (global)
    # 
    echo "Rule 40 (global)"
    # 
    $IPTABLES -N Cid1515316X29460.0
    $IPTABLES -A INPUT -p tcp -m tcp  -d ! 192.168.1.0/24   --dport 80  -j Cid1515316X29460.0
    $IPTABLES -A Cid1515316X29460.0  -s 22.22.22.22   -j DROP
    $IPTABLES -A Cid1515316X29460.0  -s 22.22.23.23   -j DROP
    $IPTABLES -A Cid1515316X29460.0  -s 192.168.1.1   -j DROP
    $IPTABLES -A Cid1515316X29460.0  -s 192.168.2.1   -j DROP
    $IPTABLES -N Cid1515316X29460.1
    $IPTABLES -A OUTPUT -p tcp -m tcp  -d ! 192.168.1.0/24   --dport 80  -j Cid1515316X29460.1
    $IPTABLES -A Cid1515316X29460.1  -s 22.22.22.22   -j DROP
    $IPTABLES -A Cid1515316X29460.1  -s 22.22.23.23   -j DROP
    $IPTABLES -A Cid1515316X29460.1  -s 192.168.1.1   -j DROP
    $IPTABLES -A Cid1515316X29460.1  -s 192.168.2.1   -j DROP
    # 
    # Rule 41 (global)
    # 
    echo "Rule 41 (global)"
    # 
    $IPTABLES -N Cid1515397X29460.0
    $IPTABLES -A OUTPUT -p tcp -m tcp  -s ! 192.168.1.0/24   --dport 80  -j Cid1515397X29460.0
    $IPTABLES -A Cid1515397X29460.0  -d 22.22.22.22   -j DROP
    $IPTABLES -A Cid1515397X29460.0  -d 22.22.23.23   -j DROP
    $IPTABLES -A Cid1515397X29460.0  -d 192.168.1.1   -j DROP
    $IPTABLES -A Cid1515397X29460.0  -d 192.168.2.1   -j DROP
    $IPTABLES -N Cid1515397X29460.1
    $IPTABLES -A INPUT -p tcp -m tcp  -s ! 192.168.1.0/24   --dport 80  -j Cid1515397X29460.1
    $IPTABLES -A Cid1515397X29460.1  -d 22.22.22.22   -j DROP
    $IPTABLES -A Cid1515397X29460.1  -d 22.22.23.23   -j DROP
    $IPTABLES -A Cid1515397X29460.1  -d 192.168.1.1   -j DROP
    $IPTABLES -A Cid1515397X29460.1  -d 192.168.2.1   -j DROP
}

ip_forward() {
    :
    
}

reset_all() {
    :
    reset_iptables_v4
}

block_action() {
    reset_all
}

stop_action() {
    reset_all
    $IPTABLES -P OUTPUT  ACCEPT
    $IPTABLES -P INPUT   ACCEPT
    $IPTABLES -P FORWARD ACCEPT
}

check_iptables() {
    IP_TABLES="$1"
    [ ! -e $IP_TABLES ] && return 151
    NF_TABLES=$(cat $IP_TABLES 2>/dev/null)
    [ -z "$NF_TABLES" ] && return 152
    return 0
}
status_action() {
    check_iptables "/proc/net/ip_tables_names"
    ret_ipv4=$?
    check_iptables "/proc/net/ip6_tables_names"
    ret_ipv6=$?
    [ $ret_ipv4 -eq 0 -o $ret_ipv6 -eq 0 ] && return 0
    [ $ret_ipv4 -eq 151 -o $ret_ipv6 -eq 151 ] && {
        echo "iptables modules are not loaded"
    }
    [ $ret_ipv4 -eq 152 -o $ret_ipv6 -eq 152 ] && {
        echo "Firewall is not configured"
    }
    exit 3
}

# See how we were called.
# For backwards compatibility missing argument is equivalent to 'start'

cmd=$1
test -z "$cmd" && {
    cmd="start"
}

case "$cmd" in
    start)
        log "Activating firewall script generated Sun Mar 18 21:16:07 2012 by vadim"
        check_tools
        
        check_run_time_address_table_files
        
        load_modules "nat "
        configure_interfaces
        verify_interfaces
         prolog_commands 
         reset_all 
        
        script_body
        ip_forward
        epilog_commands
        RETVAL=$?
        ;;

    stop)
        stop_action
        RETVAL=$?
        ;;

    status)
        status_action
        RETVAL=$?
        ;;

    block)
        block_action
        RETVAL=$?
        ;;

    reload)
        $0 stop
        $0 start
        RETVAL=$?
        ;;

    interfaces)
        configure_interfaces
        RETVAL=$?
        ;;

    test_interfaces)
        FWBDEBUG="echo"
        configure_interfaces
        RETVAL=$?
        ;;



    *)
        echo "Usage $0 [start|stop|status|block|reload|interfaces|test_interfaces]"
        ;;

esac

exit $RETVAL