!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v5.0.1.3581
!
!  Generated Wed Oct 19 16:51:04 2011 PDT by vadim
!
! Compiled for pix 6.3
! Outbound ACLs: not supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: no
! Assume firewall is part of any: yes
!
!# files: * firewall2.fw
!
! lots of different combinations of objects in the NAT rules

! C firewall2:Policy:1: warning: Rule with direction 'Outbound' was suppressed because generation of outbound access lists is turned off in firewall object settings

!
! Prolog script:
!

!
! End of prolog script:
!




nameif eth0 inside security100

nameif eth1 outside security0

nameif eth2 dmz security50


no logging buffered
no logging console
no logging timestamp
no logging on



telnet timeout 5

clear ssh
aaa authentication ssh console LOCAL
ssh timeout 5

clear snmp-server
no snmp-server enable traps

clear ntp


no service resetinbound
no service resetoutside
no sysopt connection timewait
no sysopt nodnsalias inbound
no sysopt nodnsalias outbound
floodguard disable


!################

clear xlate
clear static
clear global
clear nat
clear access-list
clear icmp
clear telnet
clear object-group

object-group service id3D6EF08C.srv.tcp.0 tcp
  port-object eq 80
  port-object eq 119
exit

object-group network id3D8FCCDE.src.net.0
  network-object host 192.168.1.10 
  network-object host 192.168.1.20 
exit

! 
! Rule  0 (eth1)
! Anti-spoofing rule
access-list outside_acl_in deny   ip host 192.168.1.1 any log 6 interval 300
access-list outside_acl_in deny   ip host 22.22.22.22 any log 6 interval 300
access-list outside_acl_in deny   ip host 192.168.2.1 any log 6 interval 300
access-list outside_acl_in deny   ip 192.168.1.0 255.255.255.0 any log 6 interval 300
! 
! Rule  1 (eth1)
! Anti-spoofing rule
! firewall2:Policy:1: warning: Rule with direction 'Outbound' was suppressed because generation of outbound access lists is turned off in firewall object settings

access-list inside_acl_in deny   ip 192.168.1.0 255.255.255.0 any log 6 interval 300
! 
! Rule  2 (global)
access-list inside_acl_in permit tcp any host 192.168.1.10 object-group id3D6EF08C.srv.tcp.0 
access-list outside_acl_in permit tcp any host 22.22.22.22 eq 80 
access-list outside_acl_in permit tcp any host 22.22.22.22 eq 119 
access-list outside_acl_in permit tcp any host 192.168.1.10 object-group id3D6EF08C.srv.tcp.0 
access-list dmz_acl_in permit tcp any host 192.168.1.10 object-group id3D6EF08C.srv.tcp.0 
! 
! Rule  3 (global)
access-list inside_acl_in permit ip object-group id3D8FCCDE.src.net.0 host 200.200.200.200 
! 
! Rule  4 (global)
access-list outside_acl_in permit ip host 200.200.200.200 object-group id3D8FCCDE.src.net.0 
! 
! Rule  6 (global)
access-list inside_acl_in deny   ip any any 
access-list outside_acl_in deny   ip any any 
access-list dmz_acl_in deny   ip any any 


access-group dmz_acl_in in interface dmz
access-group inside_acl_in in interface inside
access-group outside_acl_in in interface outside

! 
! Rule  0 (NAT)

access-list nat0.inside permit ip 192.168.1.0 255.255.255.0 192.168.2.0 255.255.255.0
nat (inside) 0 access-list nat0.inside
! 
! Rule  1 (NAT)
static (inside,dmz) 192.168.1.0 192.168.1.0 netmask 255.255.255.0
! 
! Rule  2 (NAT)
global (outside) 1 interface
access-list id3AFB66C8.0 permit ip 192.168.1.0 255.255.255.0  any 
global (dmz) 1 interface
! 
! 
! Rule  3 (NAT)
access-list id3AFB66C8.0 permit ip host 192.168.1.10   any 
! 
access-list id3AFB66C8.0 permit ip host 192.168.1.20   any 
! 
! 
! Rule  4 (NAT)
access-list id3AFB66C8.0 permit ip host 192.168.1.11   any 
! 
access-list id3AFB66C8.0 permit ip 192.168.1.12 255.255.255.252  any 
! 
! 
! Rule  5 (NAT)
access-list id3D1C2292.0 permit ip 192.168.2.0 255.255.255.0  any 
nat (dmz) 1 access-list id3D1C2292.0 0 0
! 
! Rule  6 (NAT)
! 
! 
! Rule  7 (NAT)
global (outside) 1 interface
! 
! 
! Rule  8 (NAT)
! 
! 
! Rule  9 (NAT)
! 
! 
! 
! Rule  10 (NAT)
global (outside) 1 22.22.22.0 netmask 255.255.255.0
! 
! 
! Rule  11 (NAT)
global (outside) 1 22.22.22.21-22.22.22.25 netmask 255.255.255.0
! 
! 
! 
! Rule  12 (NAT)
global (dmz) 1 interface
access-list id3D1C1104.0 permit ip host 192.168.1.10   192.168.2.0 255.255.255.0 
! 
! Rule  13 (NAT)
access-list id3D1C1D30.0 permit ip 192.168.1.0 255.255.255.0  192.168.2.0 255.255.255.0 
nat (inside) 1 access-list id3D1C1D30.0 0 0
! 
! Rule  14 (NAT)
! 
! 
! Rule  16 (NAT)
access-list id3D1BFFA4.0 permit ip host 192.168.1.10   any 
static (inside,outside) interface  access-list id3D1BFFA4.0 0 0
! 
! Rule  17 (NAT)
access-list id3D1C0835.0 permit tcp host 192.168.1.10  eq 6667  any 
static (inside,outside) tcp interface 6667  access-list id3D1C0835.0 0 0
! 
! Rule  18 (NAT)
access-list id16986X27842.0 permit tcp host 192.168.1.1  eq 6667  any 
static (inside,outside) tcp interface 6667  access-list id16986X27842.0 0 0
! 
! Rule  19 (NAT)
access-list id414351C7.0 permit tcp host 192.168.1.10  eq 80  any 
! 
! Rule  20 (NAT)
access-list id414351C7.0 permit tcp host 192.168.1.10  eq 80  any 
static (inside,outside) tcp interface 80  access-list id414351C7.0 0 0
! 
! Rule  21 (NAT)
access-list id3AFB69BD.0 permit ip host 192.168.1.10   any 
static (inside,outside) interface  access-list id3AFB69BD.0 0 0
! 
! Rule  22 (NAT)
access-list id3D1BFFCE.0 permit ip 192.168.1.0 255.255.255.0  any 
static (inside,outside) 22.22.22.0  access-list id3D1BFFCE.0 0 0
! 
! Rule  24 (NAT)
access-list id3D1BFFF6.0 permit ip host 192.168.1.10   192.168.2.0 255.255.255.0 
static (inside,dmz) interface  access-list id3D1BFFF6.0 0 0
! 
! Rule  25 (NAT)
access-list id3BEEF6D2.0 permit tcp host 192.168.1.10  eq 119  any 
static (inside,outside) tcp interface 119  access-list id3BEEF6D2.0 0 0
! 
! Rule  27 (NAT)
access-list id3B7313C4.0 permit tcp host 192.168.1.10  eq 3128  any 
static (inside,outside) tcp interface 80  access-list id3B7313C4.0 0 0
! 
! Rule  28 (NAT)
access-list id47B6CF3421818.0 permit tcp host 192.168.1.10  eq 3128  any 
! 
! Rule  29 (NAT)
access-list id36573X14603.0 permit tcp host 192.168.1.10  eq 3128  any 
static (inside,outside) tcp interface 80  access-list id36573X14603.0 0 0
! 
! Rule  30 (NAT)
access-list id47B6CF3421818.0 permit tcp host 192.168.1.10  eq 3128  any 
static (inside,outside) tcp interface 80  access-list id47B6CF3421818.0 0 0



!
! Epilog script:
!

! End of epilog script:
!
