


# 
# Rule  1 (NAT)
nat on  eth0 from 192.168.1.0/24 to any -> (eth0) 

# 
# Rule  0 (eth0)
block in   log  quick on eth0 inet  from any  to 192.168.1.255 
# 
# Rule  1 (lo)
pass  quick on lo inet  from any  to any keep state 
# 
# Rule  3 (global)
pass  quick inet proto udp  from any  to 192.168.1.255 port 68 keep state 
# 
# Rule  4 (global)
block  log  quick inet  from any  to any 
# 
# Rule  fallback rule
#    fallback rule 
block  quick inet  from any  to any 

