## -*- mode: shell-script; -*- 
##
## See http://www.cisco.com/en/US/products/hw/modules/ps2706/products_configuration_example09186a00808b4d9f.shtml
##
## Cisco says: 
## "Note: NTP cannot be configured on FWSM, because it takes its settings from the Switch."

