: Saved
:
PIX Version 7.2(1) 
!
terminal width 511
hostname pix1
domain-name some-domain.org
enable password XXXXXXXXXXXXXXXX encrypted
names
name 1.2.3.4 gw
name 192.168.3.0 fake_network
name 192.168.4.1 inside_ip
!
dns-guard
!
interface Ethernet0
 no nameif
 no security-level
 no ip address
!
interface Ethernet0.101
 vlan 101
 nameif outside
 security-level 0
 ip address 192.0.2.253 255.255.255.0 
!
interface Ethernet0.102
 vlan 102
 nameif dmz20 
 security-level 20
 ip address 10.0.0.253 255.255.255.0 standby 10.0.0.254 
!
interface Ethernet1
 speed 100
 duplex full
 nameif inside
 security-level 100
 ip address 10.1.1.206 255.255.255.0 
!
interface Ethernet2
 shutdown
 description LAN/STATE Failover Interface
 speed 10
!
interface Ethernet3
 shutdown
 no nameif
 no security-level
 no ip address
!
interface Ethernet4
 shutdown
 no nameif
 no security-level
 no ip address
!             
interface Ethernet5
 shutdown
 no nameif
 no security-level
 no ip address
!
interface Ethernet6
!
passwd MMMMMMMMMMMMMMMM encrypted
boot system flash:/pix721.bin
ftp mode passive
clock timezone PDT -7
dns server-group DefaultDNS
 domain-name some-domain.org
object-group network outside.id12051X6282.src.net.0
 network-object host 10.1.1.206
 network-object host 10.1.1.207
object-group network outside.id12051X6282.src.net.1
 network-object host 172.17.1.253
 network-object host 172.17.1.254
 network-object host 192.0.2.253
 network-object host 192.0.2.254
object-group network outside.id12051X6282.src.net.2
 network-object host 10.0.0.253
 network-object host 10.0.0.254

object-group network network-zone-inside
 network-object 10.1.1.0 255.255.255.0
object-group network network-zone-dmz20
 network-object 10.0.0.0 255.255.255.0


access-list outside_in extended deny ip object-group outside.id12051X6282.src.net.0 any log warnings 
access-list outside_in extended deny ip object-group outside.id12051X6282.src.net.1 any log warnings 
access-list outside_in extended deny ip object-group outside.id12051X6282.src.net.2 any log warnings 
access-list outside_in extended deny ip 10.1.1.0 255.255.255.0 any log warnings 
access-list inside_out extended permit udp object-group outside.id12051X6282.src.net.0 10.1.1.0 255.255.255.0 eq domain log warnings 
access-list inside_out extended permit udp object-group outside.id12051X6282.src.net.1 10.1.1.0 255.255.255.0 eq domain log warnings 
access-list inside_out extended permit udp object-group outside.id12051X6282.src.net.2 10.1.1.0 255.255.255.0 eq domain log warnings 
access-list inside_out extended permit ip 10.1.1.0 255.255.255.0 any 
access-list inside_out extended deny ip any any log warnings 
access-list inside_in extended deny ip any object-group outside.id12051X6282.src.net.0 log warnings 
access-list inside_in extended deny ip any object-group outside.id12051X6282.src.net.1 log warnings 
access-list inside_in extended deny ip any object-group outside.id12051X6282.src.net.2 log warnings 
access-list inside_in extended permit ip 10.1.1.0 255.255.255.0 any 
access-list inside_in extended deny ip any any log warnings 

access-list id12251X6282.0 extended permit ip 10.1.1.0 255.255.255.0 any 

access-list id12594X2458.0 permit tcp host 10.1.1.43 eq www any 

! example from cisco docs, see also nat command below
access-list WEB permit tcp 10.1.1.0 255.255.255.0 4.2.2.1 255.255.255.255 eq 80

access-list WEB2 permit tcp 192.168.2.0 255.255.255.0 4.2.2.1 255.255.255.255 eq 80
access-list WEB2 permit tcp 192.168.3.0 255.255.255.0 4.2.2.1 255.255.255.255 eq 80

access-list NET1 permit ip host 10.1.1.20 host 4.2.2.1


pager lines 24
logging enable
logging emblem
logging trap debugging
logging history informational
logging facility 16
logging queue 10
logging device-id ipaddress inside
logging host inside 192.168.240.20
logging host inside 10.1.1.40 format emblem
logging class config buffered debugging 
mtu outside 1500
mtu dmz20 1500
mtu inside 1500
failover
failover lan unit primary
failover lan interface failover Ethernet2
failover lan enable
failover key *****
failover link failover Ethernet2
failover interface ip failover 172.17.1.253 255.255.255.252 standby 172.17.1.254
no asdm history enable
arp timeout 14400

nat-control
global (outside) 1 interface
nat (inside) 1 access-list id12251X6282.0

global (outside) 2 192.0.2.10
global (outside) 2 192.0.2.11-192.0.2.15
global (outside) 2 192.0.2.128 netmask 255.255.255.240
global (dmz20) 2 10.0.0.128 netmask 255.255.255.240
global (outside) 3 192.0.2.20
global (outside) 3 192.0.2.30-192.0.2.31

nat (inside) 2 10.1.1.1 255.255.255.255
nat (inside) 2 10.1.1.32 255.255.255.240

nat (inside) 1 access-list WEB
nat (inside) 1 access-list WEB2

! multiple address blocks in pool 3 and multiple lines in access list WEB2
nat (inside) 3 access-list WEB2
  
static (inside,dmz20) 10.0.0.16 10.1.1.16 netmask 255.255.255.240
static (inside,dmz20) 10.0.0.100 10.1.1.100 netmask 255.255.255.255
static (inside,dmz20) interface 10.1.1.111
static (inside,outside) tcp 10.5.80.16 80 10.1.1.16 8080  netmask 255.255.255.240 0 0
static (inside,outside) tcp 10.5.80.200 80 10.10.1.200 8080  netmask 255.255.255.255 0 0

static (inside,outside) tcp 10.5.80.16 aol 10.1.1.16 aol
static (inside,outside) tcp 10.5.80.16 bgp 10.1.1.16 bgp
static (inside,outside) tcp 10.5.80.16 chargen 10.1.1.16 chargen
static (inside,outside) tcp 10.5.80.16 cifs 10.1.1.16 cifs
static (inside,outside) tcp 10.5.80.16 citrix-ica 10.1.1.16 citrix-ica
static (inside,outside) tcp 10.5.80.16 cmd 10.1.1.16 cmd
static (inside,outside) tcp 10.5.80.16 ctiqbe 10.1.1.16 ctiqbe
static (inside,outside) tcp 10.5.80.16 daytime 10.1.1.16 daytime
static (inside,outside) tcp 10.5.80.16 discard 10.1.1.16 discard
static (inside,outside) tcp 10.5.80.16 domain 10.1.1.16 domain
static (inside,outside) tcp 10.5.80.16 echo 10.1.1.16 echo
static (inside,outside) tcp 10.5.80.16 exec 10.1.1.16 exec
static (inside,outside) tcp 10.5.80.16 finger 10.1.1.16 finger
static (inside,outside) tcp 10.5.80.16 ftp 10.1.1.16 ftp
static (inside,outside) tcp 10.5.80.16 ftp-data 10.1.1.16 ftp-data
static (inside,outside) tcp 10.5.80.16 gopher 10.1.1.16 gopher
static (inside,outside) tcp 10.5.80.16 h323 10.1.1.16 h323
static (inside,outside) tcp 10.5.80.16 hostname 10.1.1.16 hostname
static (inside,outside) tcp 10.5.80.16 http 10.1.1.16 http
static (inside,outside) tcp 10.5.80.16 https 10.1.1.16 https
static (inside,outside) tcp 10.5.80.16 ident 10.1.1.16 ident
static (inside,outside) tcp 10.5.80.16 imap4 10.1.1.16 imap4
static (inside,outside) tcp 10.5.80.16 irc 10.1.1.16 irc
static (inside,outside) tcp 10.5.80.16 kerberos 10.1.1.16 kerberos
static (inside,outside) tcp 10.5.80.16 klogin 10.1.1.16 klogin
static (inside,outside) tcp 10.5.80.16 kshell 10.1.1.16 kshell
static (inside,outside) tcp 10.5.80.16 ldap 10.1.1.16 ldap
static (inside,outside) tcp 10.5.80.16 ldaps 10.1.1.16 ldaps
static (inside,outside) tcp 10.5.80.16 login 10.1.1.16 login
static (inside,outside) tcp 10.5.80.16 lotusnotes 10.1.1.16 lotusnotes
static (inside,outside) tcp 10.5.80.16 lpd 10.1.1.16 lpd
static (inside,outside) tcp 10.5.80.16 netbios-ssn 10.1.1.16 netbios-ssn
static (inside,outside) tcp 10.5.80.16 nntp 10.1.1.16 nntp
static (inside,outside) tcp 10.5.80.16 pcanywhere-data 10.1.1.16 pcanywhere-data
static (inside,outside) tcp 10.5.80.16 pim-auto-rp 10.1.1.16 pim-auto-rp
static (inside,outside) tcp 10.5.80.16 pop2 10.1.1.16 pop2
static (inside,outside) tcp 10.5.80.16 pop3 10.1.1.16 pop3
static (inside,outside) tcp 10.5.80.16 pptp 10.1.1.16 pptp
static (inside,outside) tcp 10.5.80.16 rsh 10.1.1.16 rsh
static (inside,outside) tcp 10.5.80.16 rtsp 10.1.1.16 rtsp
static (inside,outside) tcp 10.5.80.16 sip 10.1.1.16 sip
static (inside,outside) tcp 10.5.80.16 smtp 10.1.1.16 smtp
static (inside,outside) tcp 10.5.80.16 sqlnet 10.1.1.16 sqlnet
static (inside,outside) tcp 10.5.80.16 ssh 10.1.1.16 ssh
static (inside,outside) tcp 10.5.80.16 sunrpc 10.1.1.16 sunrpc
static (inside,outside) tcp 10.5.80.16 tacacs 10.1.1.16 tacacs
static (inside,outside) tcp 10.5.80.16 talk 10.1.1.16 talk
static (inside,outside) tcp 10.5.80.16 telnet 10.1.1.16 telnet
static (inside,outside) tcp 10.5.80.16 uucp 10.1.1.16 uucp
static (inside,outside) tcp 10.5.80.16 whois 10.1.1.16 whois
static (inside,outside) tcp 10.5.80.16 www 10.1.1.16 www




static (inside,outside) tcp interface www access-list id12594X2458.0 0 0 
static (inside,outside) tcp interface 80 access-list id12594X2458.0 0 0 
static (inside,outside) interface access-list id12594X2458.0 0 0 

static (inside,outside) 192.0.2.15 access-list NET1

! acl WEB2 has multiple lines. Does this even make sense ?
static (inside,outside) 192.0.2.15 access-list WEB2


access-group outside_in in interface outside
access-group inside_in in interface inside
access-group inside_out out interface inside


route inside 192.168.10.0 255.255.255.0 10.1.1.254 1
route inside 10.1.2.0 255.255.255.0 10.1.1.201 1
timeout xlate 3:00:00
timeout conn 1:00:00 half-closed 0:10:00 udp 0:02:00 icmp 0:00:02
timeout sunrpc 0:10:00 h323 0:05:00 h225 1:00:00 mgcp 0:05:00 mgcp-pat 0:05:00
timeout sip 0:30:00 sip_media 0:02:00 sip-invite 0:03:00 sip-disconnect 0:02:00
timeout uauth 2:00:00 absolute
aaa-server TACACS+ protocol tacacs+
aaa-server RADIUS protocol radius
username fwbtest password AAAAAAAAAAAAAAAA encrypted privilege 15
aaa authentication ssh console LOCAL 
snmp-server host inside 10.1.1.180 community public
snmp-server host inside 10.1.1.30 community public
snmp-server host inside 10.1.1.40 poll community public version 2c
no snmp-server location
no snmp-server contact
snmp-server community public
crypto ipsec transform-set spde esp-des esp-sha-hmac 
crypto map spdemap 21 set peer 192.0.2.254 
crypto map spdemap 21 set transform-set spde
crypto isakmp identity address 
crypto isakmp policy 21
 authentication pre-share
 encryption des
 hash sha
 group 1
 lifetime 3600
crypto isakmp policy 65535
 authentication pre-share
 encryption 3des
 hash sha
 group 2
 lifetime 86400
tunnel-group 192.0.2.254 type ipsec-l2l
tunnel-group 192.0.2.254 ipsec-attributes
 pre-shared-key *
telnet timeout 5
ssh scopy enable
ssh 10.1.1.0 255.255.255.0 inside
ssh 10.1.2.0 255.255.255.0 inside
ssh 192.0.2.100 255.255.255.255 outside
ssh timeout 20
console timeout 0
!
class-map custom_h323_h225_inspection
 match port tcp range h323 1721
class-map custom_http_inspection
 match port tcp range www 88
class-map inspection_default
 match default-inspection-traffic
!
!
policy-map type inspect dns migrated_dns_map_1
 parameters   
  message-length maximum 512
policy-map global_policy
 class inspection_default
  inspect dns migrated_dns_map_1 
  inspect ftp 
  inspect h323 h225 
  inspect h323 ras 
  inspect http 
  inspect netbios 
  inspect rsh 
  inspect rtsp 
  inspect skinny 
  inspect sqlnet 
  inspect sunrpc 
  inspect tftp 
  inspect sip 
  inspect xdmcp 
  inspect ctiqbe 
  inspect icmp 
  inspect ils 
  inspect mgcp 
  inspect esmtp 
 class custom_h323_h225_inspection
  inspect h323 h225 
 class custom_http_inspection
  inspect http 
!
service-policy global_policy global
prompt hostname context 
Cryptochecksum:xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
: end

