!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v5.0.1.3581
!
!  Generated Wed Oct 19 16:51:03 2011 PDT by vadim
!
! Compiled for pix 6.3
! Outbound ACLs: not supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: no
! Assume firewall is part of any: no
!
!# files: * firewall14.fw
!
! testing dual NAT per user's request



!
! Prolog script:
!

!
! End of prolog script:
!




nameif eth0 outside security0

nameif eth2 inside security100


no logging buffered
no logging console
no logging timestamp
no logging on


timeout xlate 3:0:0 
timeout conn 1:0:0 
timeout udp 0:2:0 
timeout rpc 0:10:0 
timeout h323 0:5:0 
timeout sip 0:30:0 
timeout sip_media 0:2:0 
timeout uauth 2:0:0 absolute 

telnet timeout 5

aaa authentication ssh console LOCAL
ssh timeout 5

no snmp-server enable traps




no service resetinbound
no service resetoutside
no sysopt connection timewait
no sysopt nodnsalias inbound
no sysopt nodnsalias outbound
floodguard enable


!################





! 
! Rule  0 (global)
access-list inside_acl_in permit ip 10.1.2.0 255.255.255.0 any 
! 
! Rule  1 (global)
access-list outside_acl_in deny   ip any any 
access-list inside_acl_in deny   ip any any 


access-group inside_acl_in in interface inside
access-group outside_acl_in in interface outside

! 
! Rule  0 (NAT)
global (outside) 1 interface
access-list id3FA74FDE.0 permit ip host 10.1.2.27   any 
nat (inside) 1 access-list id3FA74FDE.0 0 0
! 
! Rule  1 (NAT)
access-list id3FA74FCE.0 permit ip host 209.165.201.11   any 
static (outside,inside) interface  access-list id3FA74FCE.0 0 0
! 
! Rule  2 (NAT)
access-list id3FA7502F.0 permit ip host 10.1.2.27   any 
static (inside,outside) interface  access-list id3FA7502F.0 0 0



!
! Epilog script:
!

! End of epilog script:
!
