!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_iosacl v5.0.1.3584
!
!  Generated Tue Nov  8 08:41:20 2011 PST by vadim
!
! Compiled for iosacl 12.3
!
!# files: * testios20-v12.3.fw
!

! testios20-v12.3:Policy:10: error: IP options match requires IOS v12.4 or later.
! testios20-v12.3:Policy:10: error: IP options match requires IOS v12.4 or later.
! testios20-v12.3:Policy:10: error: IP options match requires IOS v12.4 or later.
! testios20-v12.3:Policy:10: error: IP options match requires IOS v12.4 or later.
! testios20-v12.3:Policy:11: error: IP options match requires IOS v12.4 or later.

!
! Prolog script:
!

!
! End of prolog script:
!

hostname testios20-v12.3

no ip access-list extended e0_in
no ip access-list extended e0_out
no ip access-list extended e1_in
no ip access-list extended e1_out

! ================ IPv4


ip access-list extended e0_in
! 
! Rule  0 (global)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  2 (ethernet0)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  3 (global)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  5 (ethernet0)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  6 (global)
  permit ip  any  any  tos 16
! 
! Rule  7 (global)
  permit ip  any  any  dscp 16
! 
! Rule  8 (global)
  permit ip  any  any  dscp af11
! 
! Rule  9 (global)
  permit ip  any  any  dscp 16
  permit ip  any  any  dscp af11
! 
! Rule  10 (ethernet0)
  permit ip  any  any  option lsr
  permit ip  any  any  option record-route
  permit ip  any  any  option ssr
  permit ip  any  any  
! 
! Rule  11 (ethernet0)
  permit ip  any  any  option any-options 
! 
! Rule  12 (global)
  permit ip  any  any  
! 
! Rule  13 (global)
  deny   ip  any  any  log 
exit

ip access-list extended e0_out
! 
! Rule  2 (ethernet0)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  6 (global)
  permit ip  any  any  tos 16
! 
! Rule  7 (global)
  permit ip  any  any  dscp 16
! 
! Rule  8 (global)
  permit ip  any  any  dscp af11
! 
! Rule  9 (global)
  permit ip  any  any  dscp 16
  permit ip  any  any  dscp af11
! 
! Rule  12 (global)
  permit ip  any  any  
! 
! Rule  13 (global)
  deny   ip  any  any  log 
exit

ip access-list extended e1_in
! 
! Rule  0 (global)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  1 (ethernet1)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  3 (global)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  4 (ethernet1)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  6 (global)
  permit ip  any  any  tos 16
! 
! Rule  7 (global)
  permit ip  any  any  dscp 16
! 
! Rule  8 (global)
  permit ip  any  any  dscp af11
! 
! Rule  9 (global)
  permit ip  any  any  dscp 16
  permit ip  any  any  dscp af11
! 
! Rule  12 (global)
  permit ip  any  any  
! 
! Rule  13 (global)
  deny   ip  any  any  log 
exit

ip access-list extended e1_out
! 
! Rule  0 (global)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  1 (ethernet1)
  permit ip  any  10.10.10.0 0.0.0.255 
  permit ip  any  10.10.11.0 0.0.0.255 
  permit ip  any  10.10.12.0 0.0.0.255 
! 
! Rule  6 (global)
  permit ip  any  any  tos 16
! 
! Rule  7 (global)
  permit ip  any  any  dscp 16
! 
! Rule  8 (global)
  permit ip  any  any  dscp af11
! 
! Rule  9 (global)
  permit ip  any  any  dscp 16
  permit ip  any  any  dscp af11
! 
! Rule  12 (global)
  permit ip  any  any  
! 
! Rule  13 (global)
  deny   ip  any  any  log 
exit


interface ethernet0
  ip access-group e0_in in
exit
interface ethernet0
  ip access-group e0_out out
exit
interface ethernet1
  ip access-group e1_in in
exit
interface ethernet1
  ip access-group e1_out out
exit





!
! Epilog script:
!

! End of epilog script:
!
