!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_iosacl v5.0.1.3584
!
!  Generated Tue Nov  8 08:41:19 2011 PST by vadim
!
! Compiled for iosacl 12.1
!
!# files: * c3620.fw
!



!
! Prolog script:
!

!
! End of prolog script:
!

no service timestamp log datetime localtime
logging buffered 6
logging console 6

no ip access-list extended e1_0_in
no ip access-list extended e1_0_out
no ip access-list extended e1_1_in
no ip access-list extended e1_1_out
no ip access-list extended fe0_0_in
no ip access-list extended fe0_0_out

! ================ IPv4


ip access-list extended e1_0_in
! 
! Rule  -1 backup ssh access rule (automatic)
   remark -1 backup ssh access rule (automatic)
  permit tcp  host 10.3.14.41 host 10.3.14.201 eq 22 
  permit tcp  host 10.3.14.41 host 192.168.171.2 eq 22 
! 
! Rule  1 (Ethernet1/0)
! this comment has empty lines at the end
! 
   remark 1 (Ethernet1/0)
   remark this comment has empty lines at the end
  permit tcp  any  any  eq 80 
! 
! Rule  2 (Ethernet1/0)
! this comment has empty line in the middle
! 
! last line
   remark 2 (Ethernet1/0)
   remark this comment has empty line in the middle
   remark last line
  permit tcp  any  any  eq 443 
! 
! Rule  5 (Ethernet1/0)
   remark 5 (Ethernet1/0)
  permit ip  any  10.3.14.0 0.0.0.255 
! 
! Rule  7 (global)
   remark 7 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  8 (global)
   remark 8 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 eq 22 
  permit udp  any  10.3.14.0 0.0.0.255 eq 53 
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  9 (global)
   remark 9 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  10 (global)
   remark 10 (global)
  permit tcp  any  eq 80 10.3.14.0 0.0.0.255 established 
exit

ip access-list extended e1_0_out
! 
! Rule  -2 backup ssh access rule (out) (automatic)
   remark -2 backup ssh access rule (out) (automatic)
  permit tcp  host 10.3.14.201 eq 22 host 10.3.14.41 
  permit tcp  host 192.168.171.2 eq 22 host 10.3.14.41 
! 
! Rule  1 (Ethernet1/0)
! this comment has empty lines at the end
! 
   remark 1 (Ethernet1/0)
   remark this comment has empty lines at the end
  permit tcp  any  any  eq 80 
! 
! Rule  2 (Ethernet1/0)
! this comment has empty line in the middle
! 
! last line
   remark 2 (Ethernet1/0)
   remark this comment has empty line in the middle
   remark last line
  permit tcp  any  any  eq 443 
! 
! Rule  4 (Ethernet1/0)
! this comment ends with a whitespace  
   remark 4 (Ethernet1/0)
   remark this comment ends with a whitespace
  permit ip  10.3.14.0 0.0.0.255 any  
exit

ip access-list extended e1_1_in
! 
! Rule  -1 backup ssh access rule (automatic)
   remark -1 backup ssh access rule (automatic)
  permit tcp  host 10.3.14.41 host 10.3.14.201 eq 22 
  permit tcp  host 10.3.14.41 host 192.168.171.2 eq 22 
! 
! Rule  0 (Ethernet1/1)
! interface eth 1/1 has only
! inbound access list
   remark 0 (Ethernet1/1)
   remark interface eth 1/1 has only
   remark inbound access list
  permit tcp  any  any  eq 80 
! 
! Rule  7 (global)
   remark 7 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  8 (global)
   remark 8 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 eq 22 
  permit udp  any  10.3.14.0 0.0.0.255 eq 53 
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  9 (global)
   remark 9 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  10 (global)
   remark 10 (global)
  permit tcp  any  eq 80 10.3.14.0 0.0.0.255 established 
exit

ip access-list extended e1_1_out
! 
! Rule  -2 backup ssh access rule (out) (automatic)
   remark -2 backup ssh access rule (out) (automatic)
  permit tcp  host 10.3.14.201 eq 22 host 10.3.14.41 
  permit tcp  host 192.168.171.2 eq 22 host 10.3.14.41 
exit

ip access-list extended fe0_0_in
! 
! Rule  -1 backup ssh access rule (automatic)
   remark -1 backup ssh access rule (automatic)
  permit tcp  host 10.3.14.41 host 10.3.14.201 eq 22 
  permit tcp  host 10.3.14.41 host 192.168.171.2 eq 22 
! 
! Rule  3 (FastEthernet0/0)
!     this comment starts with a whitespace
   remark 3 (FastEthernet0/0)
   remark this comment starts with a whitespace
  permit ip  10.3.14.0 0.0.0.255 any  
! 
! Rule  7 (global)
   remark 7 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  8 (global)
   remark 8 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 eq 22 
  permit udp  any  10.3.14.0 0.0.0.255 eq 53 
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  9 (global)
   remark 9 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  10 (global)
   remark 10 (global)
  permit tcp  any  eq 80 10.3.14.0 0.0.0.255 established 
exit

ip access-list extended fe0_0_out
! 
! Rule  -2 backup ssh access rule (out) (automatic)
   remark -2 backup ssh access rule (out) (automatic)
  permit tcp  host 10.3.14.201 eq 22 host 10.3.14.41 
  permit tcp  host 192.168.171.2 eq 22 host 10.3.14.41 
! 
! Rule  6 (FastEthernet0/0)
   remark 6 (FastEthernet0/0)
  permit ip  any  10.3.14.0 0.0.0.255 
! 
! Rule  7 (global)
   remark 7 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  8 (global)
   remark 8 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 eq 22 
  permit udp  any  10.3.14.0 0.0.0.255 eq 53 
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  9 (global)
   remark 9 (global)
  permit tcp  any  10.3.14.0 0.0.0.255 established 
! 
! Rule  10 (global)
   remark 10 (global)
  permit tcp  any  eq 80 10.3.14.0 0.0.0.255 established 
exit


interface Ethernet1/0
  ip access-group e1_0_in in
exit
interface Ethernet1/0
  ip access-group e1_0_out out
exit
interface Ethernet1/1
  ip access-group e1_1_in in
exit
interface Ethernet1/1
  ip access-group e1_1_out out
exit
interface FastEthernet0/0
  ip access-group fe0_0_in in
exit
interface FastEthernet0/0
  ip access-group fe0_0_out out
exit



! 
! Rule 0 (main)
! 
! 
! 
ip route 10.10.10.0 255.255.255.0 10.3.14.254 1
! 
! Rule 1 (main)
! 
! 
! 
ip route 10.10.11.0 255.255.255.0 FastEthernet0/0 1
! 
! Rule 2 (main)
! 
! 
! 
ip route 10.10.12.0 255.255.255.0 FastEthernet0/0 1
! 
! Rule 3 (main)
! 
! 
! 
ip route 0.0.0.0 0.0.0.0  Ethernet1/0 1

!
! Epilog script:
!

! End of epilog script:
!
