!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v5.0.1.3581
!
!  Generated Wed Oct 19 16:51:13 2011 PDT by vadim
!
! Compiled for pix 8.3
! Outbound ACLs: supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: no
! Assume firewall is part of any: yes
!
!# files: * firewall92.fw
!
! testing new style ASA 8.3 nat commands
! no-nat rules ("identity nat")



!
! Prolog script:
!

!
! End of prolog script:
!




interface FastEthernet0
  nameif inside
  security-level 100
exit

interface FastEthernet1
  nameif outside
  security-level 0
exit


no logging buffered
no logging console
no logging timestamp
no logging on


timeout xlate 3:0:0 
timeout conn 1:0:0 
timeout udp 0:2:0 
timeout sunrpc 0:10:0 
timeout h323 0:5:0 
timeout sip 0:30:0 
timeout sip_media 0:0:0 
timeout half-closed 0:0:0 
timeout uauth 2:0:0 absolute 


clear config ssh
aaa authentication ssh console LOCAL

clear config snmp-server
no snmp-server enable traps

clear config ntp


no service resetinbound
no service resetoutside
no sysopt connection timewait
no sysopt nodnsalias inbound
no sysopt nodnsalias outbound


class-map inspection_default
  match default-inspection-traffic

policy-map global_policy
  class inspection_default

service-policy global_policy global

policy-map type inspect ip-options ip-options-map
parameters
  eool action allow
  router-alert action clear


!################

clear xlate
clear config nat
clear config access-list
clear config icmp
clear config telnet
clear config object-group
clear config object

object service http.0
  service tcp destination eq 80
exit

object service smtp.0
  service tcp destination eq 25
exit

object network spamhost1.0
  host 61.150.47.112
exit

object network hostA:eth0.0
  host 192.168.1.10
exit

object network Internal_net.0
  subnet 192.168.1.0 255.255.255.0
exit

object network internal_subnet_1.0
  subnet 192.168.1.0 255.255.255.192
exit

object network internal_subnet_2.0
  subnet 192.168.1.64 255.255.255.192
exit

object network test_range_1.0
  range 192.168.1.11 192.168.1.15
exit

object-group network id20655X6113.osrc.net.0
  network-object object internal_subnet_1.0
  network-object object internal_subnet_2.0
exit

object-group network id20600X6113.osrc.net.0
  network-object object test_range_1.0
exit

! 
! Rule  0 (global)
access-list inside_acl_in deny   ip any any 
access-list outside_acl_in deny   ip any any 


access-group inside_acl_in in interface inside
access-group outside_acl_in in interface outside

! 
! Rule  0 (NAT)
nat (inside,outside) source static Internal_net.0 Internal_net.0 service http.0 http.0 description "0 (NAT)"
! 
! Rule  1 (NAT)
nat (inside,outside) source static hostA:eth0.0 hostA:eth0.0 service smtp.0 smtp.0 description "1 (NAT)"
! 
! Rule  2 (NAT)
nat (inside,outside) source static hostA:eth0.0 hostA:eth0.0 destination static spamhost1.0 spamhost1.0 service smtp.0 smtp.0 description "2 (NAT)"
! 
! Rule  3 (NAT)
nat (inside,outside) source static id20655X6113.osrc.net.0 id20655X6113.osrc.net.0 service smtp.0 smtp.0 description "3 (NAT)"
! 
! Rule  4 (NAT)
nat (inside,outside) source static id20600X6113.osrc.net.0 id20600X6113.osrc.net.0 destination static spamhost1.0 spamhost1.0 service smtp.0 smtp.0 description "4 (NAT)"



!
! Epilog script:
!

! End of epilog script:
!
