!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v5.0.1.3581
!
!  Generated Wed Oct 19 16:51:13 2011 PDT by vadim
!
! Compiled for pix 8.3
! Outbound ACLs: supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: no
! Assume firewall is part of any: yes
!
!# files: * firewall94.fw
!
! test using address ranges in policy rule



!
! Prolog script:
!

!
! End of prolog script:
!




interface Ethernet0/0
  nameif outside
  security-level 0
exit

interface Ethernet0/1
  nameif inside
  security-level 100
exit


no logging buffered
no logging console
no logging timestamp
no logging on



telnet timeout -1

clear config ssh
aaa authentication ssh console LOCAL
ssh timeout -1

clear config snmp-server
no snmp-server enable traps

clear config ntp


no service resetinbound
no service resetoutside
no sysopt connection timewait
no sysopt nodnsalias inbound
no sysopt nodnsalias outbound


class-map inspection_default
  match default-inspection-traffic

policy-map global_policy

service-policy global_policy global


!################

clear config access-list
clear config icmp
clear config telnet
clear config object-group
clear config object

object network inside-range-1.0
  range 10.0.0.5 10.0.0.10
exit

object network inside-range-2.0
  range 10.0.0.8 10.0.0.15
exit

object-group network id26782X14355.src.net.0
  network-object object inside-range-1.0
  network-object object inside-range-2.0
exit

! 
! Rule  0 (global)
access-list inside_acl_in  remark 0 (global)
access-list inside_acl_in deny   ip object-group id26782X14355.src.net.0 any log 6 interval 300


access-group inside_acl_in in interface inside





!
! Epilog script:
!

! End of epilog script:
!
