!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v4.2.0.3530
!
!  Generated Wed Apr 20 10:40:44 2011 PDT by vadim
!
! Compiled for pix 8.3
! Outbound ACLs: supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: no
! Assume firewall is part of any: yes
!
!# files: * firewall91.fw
!
! testing new style ASA 8.3 nat commands
! DNAT rules

! N firewall91:NAT:8: error: Can not translate multiple services into one service in one rule. 
! N firewall91:NAT:9: error: Translated service should be 'Original' or should contain single object.
! N firewall91:NAT:13: error: Oiginal destination can not be "any" in rules that translate destination
! N firewall91:NAT:14: error: Oiginal destination can not be "any" in rules that translate destination
! N firewall91:NAT:15: error: Oiginal destination can not be "any" in rules that translate destination
! N firewall91:NAT:16: error: Oiginal destination can not be "any" in rules that translate destination

!
! Prolog script:
!

!
! End of prolog script:
!




interface FastEthernet0
  nameif inside
  security-level 100
exit

interface FastEthernet1
  nameif outside
  security-level 0
exit


no logging buffered
no logging console
no logging timestamp
no logging on


timeout xlate 3:0:0 
timeout conn 1:0:0 
timeout udp 0:2:0 
timeout sunrpc 0:10:0 
timeout h323 0:5:0 
timeout sip 0:30:0 
timeout sip_media 0:0:0 
timeout half-closed 0:0:0 
timeout uauth 2:0:0 absolute 


clear config ssh
aaa authentication ssh console LOCAL

clear config snmp-server
no snmp-server enable traps

clear config ntp


no service resetinbound
no service resetoutside
no sysopt connection timewait
no sysopt nodnsalias inbound
no sysopt nodnsalias outbound


class-map inspection_default
  match default-inspection-traffic

policy-map global_policy
  class inspection_default

service-policy global_policy global

policy-map type inspect ip-options ip-options-map
parameters
  eool action allow
  router-alert action clear


!################

clear xlate
clear config nat
clear config access-list
clear config icmp
clear config telnet
clear config object

object service http.0
  service tcp destination eq 80
exit

object service https.0
  service tcp destination eq 443
exit

object service squid.0
  service tcp destination eq 3128
exit

object network external_gw2.0
  host 22.22.22.100
exit

object network hostA:eth0.0
  host 192.168.1.10
exit

object network internal_subnet_1.0
  subnet 192.168.1.0 255.255.255.192
exit

object network test_range_1.0
  range 192.168.1.11 192.168.1.15
exit

object network outside_range.0
  range 22.22.22.21 22.22.22.25
exit

! 
! Rule  0 (global)
access-list inside_acl_in deny   ip any any 
access-list outside_acl_in deny   ip any any 


access-group inside_acl_in in interface inside
access-group outside_acl_in in interface outside

! 
! Rule  0 (NAT)
nat (outside,inside) source static any any destination static interface hostA:eth0.0 description "0 (NAT)"
! 
! Rule  1 (NAT)
nat (outside,inside) source static any any destination static interface hostA:eth0.0 description "1 (NAT)"
! 
! Rule  2 (NAT)
nat (outside,inside) source static any any destination static external_gw2.0 hostA:eth0.0 description "2 (NAT)"
! 
! Rule  3 (NAT)
nat (outside,inside) source static any any destination static interface hostA:eth0.0 service http.0 http.0 description "3 (NAT)"
! 
! Rule  4 (NAT)
nat (outside,inside) source static any any destination static interface hostA:eth0.0 service http.0 http.0 description "4 (NAT)"
! 
! Rule  5 (NAT)
nat (outside,inside) source static any any destination static interface hostA:eth0.0 service http.0 squid.0 description "5 (NAT)"
! 
! Rule  6 (NAT)
nat (outside,inside) source static any any destination static interface hostA:eth0.0 service https.0 https.0 description "6 (NAT)"
! 
! Rule  7 (NAT)
nat (outside,inside) source static any any destination static interface hostA:eth0.0 service http.0 http.0 description "7 (NAT)"
! 
! Rule  10 (NAT)
! for #1941
nat (outside,inside) source static any any destination static outside_range.0 hostA:eth0.0 description "10 (NAT)"
! 
! Rule  11 (NAT)
! for #1941
nat (inside,outside) source dynamic internal_subnet_1.0 interface destination static outside_range.0 hostA:eth0.0 description "11 (NAT)"
! 
! Rule  12 (NAT)
! translating one range into another.
nat (outside,inside) source static any any destination static outside_range.0 test_range_1.0 description "12 (NAT)"



!
! Epilog script:
!

! End of epilog script:
!
