!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v4.2.0.3530
!
!  Generated Wed Apr 20 10:40:45 2011 PDT by vadim
!
! Compiled for pix 8.3
! Outbound ACLs: supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: no
! Assume firewall is part of any: yes
!
!# files: * firewall93.fw
!
! test for #1949
! split NAT rule by OSrc to make sure objects in OSrc match network zones of
! inetrfaces



!
! Prolog script:
!

!
! End of prolog script:
!




interface Ethernet0/0
  nameif outside
  security-level 0
exit

interface Ethernet0/1
  nameif inside
  security-level 100
exit

interface Ethernet0/2
  nameif dmz
  security-level 10
exit


no logging buffered
no logging console
no logging timestamp
no logging on


timeout xlate 0:0:30 
timeout conn 0:0:0 
timeout udp 0:0:0 
timeout sunrpc 0:0:0 
timeout h323 0:0:0 
timeout sip 0:0:0 
timeout sip_media 0:0:0 
timeout half-closed 0:0:0 
timeout uauth 0:0:0 


clear config ssh
aaa authentication ssh console LOCAL

clear config snmp-server
no snmp-server enable traps

clear config ntp


no service resetinbound
no service resetoutside
no sysopt connection timewait
no sysopt nodnsalias inbound
no sysopt nodnsalias outbound


class-map inspection_default
  match default-inspection-traffic

policy-map global_policy
  class inspection_default

service-policy global_policy global




clear xlate
clear config nat
clear config object

object network dmz-range-1.0
  range 172.16.0.10 172.16.0.15
exit

object network inside-range-1.0
  range 10.0.0.1 10.0.0.5
exit



! 
! Rule  0 (NAT)
nat (inside,outside) source dynamic inside-range-1.0 interface description "0 (NAT)"
nat (dmz,outside) source dynamic dmz-range-1.0 interface description "0 (NAT)"



!
! Epilog script:
!

! End of epilog script:
!
