## -*- mode: shell-script; -*- 
##
## To be able to make changes to the part of configuration created
## from this configlet you need to copy this file to the directory
## fwbuilder/configlets/sveasoft/ in your home directory and modify it.
## Double "##" comments are removed during processing but single "#"
## comments are be retained and appear in the generated script. Empty
## lines are removed as well.  
##
## Configlets support simple macro language with these constructs:
## {{$var}} is variable expansion
## {{if var}} is conditional operator.
##
## This configlet defines commands executed when iptables script is ran
## with command line argument "block". By default it resets iptables 
## tables and chains using function reset_all and optionally adds backup
## ssh access rules.

block_action() {
    reset_all

## it helps to add backup ssh access rule as early as possible so that
## ssh session opened from the management station won't break after
## all chains are flushed. The installation process may stall if
## stdout buffer gets filled with diagnostic or progress output from
## this script printed after chains are flushed but before a rule
## permitting ssh is installed. This may happen if script debugging is
## on or there are many NAT rules (so it prints a lot of "Rule NN
## (NAT)" lines).

{{if mgmt_access}}
    # backup ssh access
    $IPTABLES -A INPUT  -p tcp -m tcp  -s {{$ssh_management_address}}  --dport 22  -m state --state NEW,ESTABLISHED -j  ACCEPT
    $IPTABLES -A OUTPUT  -p tcp -m tcp  -d {{$ssh_management_address}}  --sport 22  -m state --state ESTABLISHED,RELATED -j ACCEPT
{{endif}}
}

