!
!  This is automatically generated file. DO NOT MODIFY !
!
!  Firewall Builder  fwb_pix v4.2.0.3530
!
!  Generated Wed Apr 20 10:40:46 2011 PDT by vadim
!
! Compiled for fwsm 2.3
! Outbound ACLs: supported
! Emulate outbound ACLs: yes
! Generating outbound ACLs: no
! Assume firewall is part of any: yes
!
!# files: * fwsm1.fw
!

! C fwsm1:Policy:18: error: Rule '18 (global)' shadows rule '20 (global)'  below it
! C fwsm1:Policy:3: warning: Rule with direction 'Outbound' was suppressed because generation of outbound access lists is turned off in firewall object settings
! C fwsm1:Policy:13: warning: MAC address matching is not supported. One or several MAC addresses removed from source in the rule

!
! Prolog script:
!

!
! End of prolog script:
!




hostname fwsm1

nameif ethernet1 outside security0

nameif ethernet0 inside security100

nameif ethernet2 dmz security50



logging host inside 192.168.1.30
logging queue 512
logging facility 16
logging trap 0
no logging buffered
no logging console
no logging timestamp
logging on


timeout xlate 3:0:0 
timeout conn 1:0:0 
timeout udp 0:2:0 
timeout rpc 0:10:0 
timeout h323 0:5:0 
timeout sip 0:30:0 
timeout sip_media 0:0:0 
timeout half-closed 0:0:0 
timeout uauth 2:0:0 absolute 

telnet timeout 5

clear ssh
aaa authentication ssh console LOCAL
ssh timeout 5

clear snmp-server
snmp-server community public
snmp-server enable traps
snmp-server host inside 192.168.1.20 poll  
snmp-server host inside 192.168.1.22 trap  




no service resetinbound
no service resetoutside
sysopt connection tcpmss 1380
sysopt nodnsalias inbound
sysopt nodnsalias outbound
floodguard disable


fixup protocol ftp 21
fixup protocol h323 h225 1720
fixup protocol h323 ras 1718-1719
fixup protocol http 80
fixup protocol ils 389
fixup protocol rsh 514
fixup protocol rtsp 554
fixup protocol sip 5060
fixup protocol skinny 2000
fixup protocol smtp 25
fixup protocol sqlnet 1521


!################
access-list mode auto

clear access-list tmp_acl
access-list tmp_acl permit ip 192.168.1.0 255.255.255.0 any 
access-list tmp_acl deny ip any any 

access-group tmp_acl in interface outside
access-group tmp_acl in interface inside
access-group tmp_acl in interface dmz

clear xlate
clear static
clear global
clear nat
clear access-list dmz_acl_in
clear access-list inside_acl_in
clear access-list outside_acl_in
clear icmp
clear telnet
clear object-group

object-group network id444A03DE9567.dst.net.0
  network-object host 211.11.11.11 
  network-object host 211.22.22.22 
exit

object-group service id444A03DE9567.srv.tcp.0 tcp
  port-object eq 113
  port-object eq 80
  port-object eq 443
  port-object eq 143
  port-object eq 25
  port-object eq 22
  port-object eq 540
exit

object-group icmp-type id444A04039567.srv.icmp.0
  icmp-object 3
  icmp-object 0
  icmp-object 11
exit

object-group service id444A040F9567.srv.tcp.0 tcp
  port-object eq 70
  port-object eq 6667
  port-object eq 3128
  port-object eq 23
exit

object-group service id444A040F9567.srv.udp.0 udp
  port-object eq 53
  port-object eq 161
exit

object-group network id444A04349567.dst.net.0
  network-object host 192.168.1.10 
  network-object host 192.168.1.20 
exit

object-group network id444A04429567.dst.net.0
  network-object 192.168.1.250 255.255.255.254 
  network-object 192.168.1.252 255.255.255.252 
exit

object-group network id444A044E9567.dst.net.0
  network-object 192.168.1.250 255.255.255.254 
  network-object 192.168.1.252 255.255.255.252 
exit

object-group network id444A04679567.dst.net.0
  network-object host 192.168.1.11 
  network-object host 192.168.1.12 
  network-object host 192.168.1.13 
  network-object host 192.168.1.14 
  network-object host 192.168.1.15 
exit

object-group service id444A04679567.srv.tcp.0 tcp
  port-object eq 113
  port-object eq 80
  port-object eq 443
  port-object eq 143
  port-object eq 25
  port-object eq 3128
  port-object eq 22
  port-object eq 540
exit

object-group network id444A04749567.dst.net.0
  network-object 192.168.1.11 255.255.255.255 
  network-object 192.168.1.12 255.255.255.252 
exit

object-group service id444A04819567.srv.tcp.0 tcp
  port-object eq 113
  port-object eq 13
  port-object eq 53
  port-object eq 2105
  port-object eq 21
  port-object eq 70
  port-object eq 80
  port-object eq 443
  port-object eq 143
  port-object eq 993
  port-object eq 6667
  port-object eq 6667
  port-object eq 543
  port-object eq 544
  port-object eq 389
  port-object eq 98
  port-object eq 3306
  port-object eq 2049
  port-object eq 119
  port-object eq 110
  port-object eq 5432
  port-object eq 515
  port-object eq 26000
  port-object eq 512
  port-object eq 513
  port-object eq 514
  port-object eq 4321
  port-object eq 25
  port-object eq 465
  port-object eq 1080
  port-object eq 3128
  port-object eq 22
  port-object eq 111
  port-object eq 23
  port-object range 10000 11000
  port-object eq 540
  port-object eq 7100
exit

! 
! Rule  2 (ethernet1)
icmp permit any 3  outside
access-list outside_acl_in permit icmp any host 22.22.22.22 3 
access-list outside_acl_in permit icmp any any 3 
! 
! Rule  3 (ethernet1)
! anti-spoofing rule
! fwsm1:Policy:3: warning: Rule with direction 'Outbound' was suppressed because generation of outbound access lists is turned off in firewall object settings

access-list inside_acl_in permit ip 192.168.1.0 255.255.255.0 any log 0 interval 300
! 
! Rule  4 (ethernet0)
ssh 192.168.1.0 255.255.255.0 inside
! 
! Rule  5 (ethernet0)
access-list inside_acl_in permit tcp any object-group id444A03DE9567.dst.net.0 object-group id444A03DE9567.srv.tcp.0 
access-list inside_acl_in permit tcp any object-group id444A03DE9567.dst.net.0 object-group id444A03DE9567.srv.tcp.0 
access-list dmz_acl_in permit tcp any object-group id444A03DE9567.dst.net.0 object-group id444A03DE9567.srv.tcp.0 
! 
! Rule  6 (ethernet0)
access-list inside_acl_in deny   ip any host 192.168.1.255 
! 
! Rule  8 (global)
access-list outside_acl_in permit icmp any host 192.168.1.10 object-group id444A04039567.srv.icmp.0 
access-list inside_acl_in permit icmp any host 192.168.1.10 object-group id444A04039567.srv.icmp.0 
access-list dmz_acl_in permit icmp any host 192.168.1.10 object-group id444A04039567.srv.icmp.0 
! 
! Rule  9 (global)
access-list outside_acl_in permit icmp any host 192.168.1.10 
access-list inside_acl_in permit icmp any host 192.168.1.10 
access-list dmz_acl_in permit icmp any host 192.168.1.10 
access-list outside_acl_in permit tcp any host 192.168.1.10 object-group id444A040F9567.srv.tcp.0 
access-list inside_acl_in permit tcp any host 192.168.1.10 object-group id444A040F9567.srv.tcp.0 
access-list dmz_acl_in permit tcp any host 192.168.1.10 object-group id444A040F9567.srv.tcp.0 
access-list outside_acl_in permit udp any host 192.168.1.10 object-group id444A040F9567.srv.udp.0 
access-list inside_acl_in permit udp any host 192.168.1.10 object-group id444A040F9567.srv.udp.0 
access-list dmz_acl_in permit udp any host 192.168.1.10 object-group id444A040F9567.srv.udp.0 
access-list outside_acl_in permit 47 any host 192.168.1.10 
access-list inside_acl_in permit 47 any host 192.168.1.10 
access-list dmz_acl_in permit 47 any host 192.168.1.10 
! 
! Rule  10 (global)
access-list outside_acl_in permit icmp any host 22.22.22.22 3 log 0 interval 300
icmp permit any 3  inside
access-list inside_acl_in permit icmp any host 192.168.1.1 3 log 0 interval 300
icmp permit any 3  dmz
access-list dmz_acl_in permit icmp any host 192.168.2.1 3 log 0 interval 300
access-list outside_acl_in permit icmp any any 3 log 0 interval 300
access-list inside_acl_in permit icmp any any 3 log 0 interval 300
access-list dmz_acl_in permit icmp any any 3 log 0 interval 300
access-list outside_acl_in permit 47 any any log 0 interval 300
access-list inside_acl_in permit 47 any any log 0 interval 300
access-list dmz_acl_in permit 47 any any log 0 interval 300
access-list outside_acl_in permit 50 any any log 0 interval 300
access-list inside_acl_in permit 50 any any log 0 interval 300
access-list dmz_acl_in permit 50 any any log 0 interval 300
! 
! Rule  12 (global)
access-list outside_acl_in permit ip object-group id444A03DE9567.dst.net.0 object-group id444A04349567.dst.net.0 
! 
! Rule  13 (global)
! fwsm1:Policy:13: warning: MAC address matching is not supported. One or several MAC addresses removed from source in the rule

access-list inside_acl_in permit tcp host 192.168.1.10 object-group id444A04429567.dst.net.0 eq 3128 
! 
! Rule  14 (global)
access-list outside_acl_in permit tcp any object-group id444A044E9567.dst.net.0 eq 3128 
access-list inside_acl_in permit tcp any object-group id444A044E9567.dst.net.0 eq 3128 
access-list dmz_acl_in permit tcp any object-group id444A044E9567.dst.net.0 eq 3128 
! 
! Rule  15 (global)
ssh 0.0.0.0 0.0.0.0 outside
ssh 0.0.0.0 0.0.0.0 inside
ssh 0.0.0.0 0.0.0.0 dmz
access-list outside_acl_in permit icmp any host 22.22.22.22 3 
access-list inside_acl_in permit icmp any host 192.168.1.1 3 
access-list dmz_acl_in permit icmp any host 192.168.2.1 3 
! 
! Rule  16 (global)
access-list outside_acl_in permit tcp any object-group id444A04679567.dst.net.0 object-group id444A04679567.srv.tcp.0 
access-list inside_acl_in permit tcp any object-group id444A04679567.dst.net.0 object-group id444A04679567.srv.tcp.0 
access-list dmz_acl_in permit tcp any object-group id444A04679567.dst.net.0 object-group id444A04679567.srv.tcp.0 
! 
! Rule  17 (global)
access-list outside_acl_in permit tcp any object-group id444A04749567.dst.net.0 object-group id444A04679567.srv.tcp.0 
access-list inside_acl_in permit tcp any object-group id444A04749567.dst.net.0 object-group id444A04679567.srv.tcp.0 
access-list dmz_acl_in permit tcp any object-group id444A04749567.dst.net.0 object-group id444A04679567.srv.tcp.0 
! 
! Rule  18 (global)
! fwsm1:Policy:18: error: Rule '18 (global)' shadows rule '20 (global)'  below it

access-list outside_acl_in permit tcp any 192.168.1.0 255.255.255.0 object-group id444A04819567.srv.tcp.0 
access-list inside_acl_in permit tcp any 192.168.1.0 255.255.255.0 object-group id444A04819567.srv.tcp.0 
access-list dmz_acl_in permit tcp any 192.168.1.0 255.255.255.0 object-group id444A04819567.srv.tcp.0 
! 
! Rule  19 (global)
! objects hostA and hostB are
! redundant and should be removed by
!  removeRedundantAddressesFromDst
access-list outside_acl_in permit tcp any 192.168.1.0 255.255.255.0 eq 1494 
access-list inside_acl_in permit tcp any 192.168.1.0 255.255.255.0 eq 1494 
access-list dmz_acl_in permit tcp any 192.168.1.0 255.255.255.0 eq 1494 
! 
! Rule  20 (global)
access-list outside_acl_in permit tcp any gt 1023 host 192.168.1.10 eq 80 
access-list inside_acl_in permit tcp any gt 1023 host 192.168.1.10 eq 80 
access-list dmz_acl_in permit tcp any gt 1023 host 192.168.1.10 eq 80 
! 
! Rule  23 (global)
access-list outside_acl_in permit ip host 22.22.22.22 host 22.22.22.22 log 0 interval 300
access-list inside_acl_in permit ip host 192.168.1.1 host 192.168.1.1 log 0 interval 300
access-list dmz_acl_in permit ip host 192.168.2.1 host 192.168.2.1 log 0 interval 300
! 
! Rule  24 (global)
access-list outside_acl_in permit ip host 22.22.22.22 any 
access-list inside_acl_in permit ip host 192.168.1.1 any 
access-list dmz_acl_in permit ip host 192.168.2.1 any 
access-list inside_acl_in permit ip 192.168.1.0 255.255.255.0 any 
! 
! Rule  25 (global)
access-list outside_acl_in deny   ip any any log 0 interval 300
access-list inside_acl_in deny   ip any any log 0 interval 300
access-list dmz_acl_in deny   ip any any log 0 interval 300


access-group dmz_acl_in in interface dmz
access-group inside_acl_in in interface inside
access-group outside_acl_in in interface outside

! 
! Rule  0 (NAT)
global (outside) 1 interface
nat (inside) 1 192.168.1.0 255.255.255.0 0 0
global (dmz) 1 interface
! 
! 
! Rule  1 (NAT)
nat (dmz) 1 0.0.0.0 0.0.0.0 0 0
! 
! Rule  2 (NAT)
nat (inside) 1 0.0.0.0 0.0.0.0 0 0
! 
! 
! Rule  3 (NAT)
global (outside) 1 22.22.22.0 netmask 255.255.255.0
! 
! 
! Rule  4 (NAT)
global (outside) 1 22.22.22.21-22.22.22.25 netmask 255.255.255.0
! 
! 
! Rule  5 (NAT)
static (inside,outside) tcp interface 25 192.168.1.10 25  0 0
! 
! Rule  6 (NAT)
global (inside) 8 interface
nat (dmz) 8 192.168.2.0 255.255.255.0 outside
! 
! Rule  7 (NAT)

clear access-list nat0.inside
access-list nat0.inside permit ip 192.168.1.0 255.255.255.0 192.168.2.0 255.255.255.0
nat (inside) 0 access-list nat0.inside
! 
! Rule  8 (NAT)

access-list nat0.inside permit ip host 192.168.1.11  192.168.2.0 255.255.255.0

access-list nat0.inside permit ip host 192.168.1.12  192.168.2.0 255.255.255.0

access-list nat0.inside permit ip host 192.168.1.13  192.168.2.0 255.255.255.0

access-list nat0.inside permit ip host 192.168.1.14  192.168.2.0 255.255.255.0

access-list nat0.inside permit ip host 192.168.1.15  192.168.2.0 255.255.255.0
! 
! Rule  9 (NAT)
nat (dmz) 0 0 0
! 
! Rule  10 (NAT)
static (inside,dmz) 192.168.1.0 192.168.1.0 netmask 255.255.255.0
! 
! Rule  11 (NAT)
static (inside,dmz) 192.168.1.10 192.168.1.10 netmask 255.255.255.255



!
! Epilog script:
!

! End of epilog script:
!
